From 145aa5dfb5b3aa0ce957e4144a4383ab1a0d5dee Mon Sep 17 00:00:00 2001
From: tilghman <tilghman@f38db490-d61c-443f-a65b-d21fe96a405b>
Date: Tue, 24 Jul 2007 18:19:18 +0000
Subject: Fix escaping and some of the formattting (closes issue #10285)

git-svn-id: http://svn.digium.com/svn/asterisk/trunk@76874 f38db490-d61c-443f-a65b-d21fe96a405b
---
 doc/tex/jitterbuffer.tex | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

(limited to 'doc/tex/jitterbuffer.tex')

diff --git a/doc/tex/jitterbuffer.tex b/doc/tex/jitterbuffer.tex
index 5122f1286..59e1474cb 100644
--- a/doc/tex/jitterbuffer.tex
+++ b/doc/tex/jitterbuffer.tex
@@ -43,7 +43,7 @@ backwards compatible architecture. Look in the source code for instructions.
 \subsubsection{Testing and monitoring}
 
 You can test the effectiveness of PLC and the new jitterbuffer's detection of loss by using 
-the new CLI command "iax2 test losspct <n>".  This will simulate n percent packet loss 
+the new CLI command "iax2 test losspct $<$n$>$".  This will simulate n percent packet loss 
 coming \_in\_ to chan\_iax2. You should find that with PLC and the new JB, 10 percent packet 
 loss should lead to just a tiny amount of distortion, while without PLC, it would lead to 
 silent gaps in your audio.
-- 
cgit v1.2.3

