<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.0">
<drawing>
<library>
<description>&lt;b&gt;PCB Matrix Packages&lt;/b&gt;&lt;p&gt;</description>
<packages>
<package name="QFN16_3X3">
</package>
<package name="AMPHENOL_SIM">
</package>
<package name="FTM-110-XX-XX-DV-S">
<description>&lt;b&gt;PCB Libraries Package&lt;b&gt;</description>
</package>
<package name="FTM-105-XX-XX-DV-S">
<description>&lt;b&gt;PCB Matrix Packages&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="FTSH-105-01-XXX-DV-K">
<description>TERMINAL STRIP, .050 inch(1.27mm) PITCH, 10 PINS, KEYED</description>
</package>
<package name="TQFP44">
<description>&lt;b&gt;Thin Quad Flat Pack&lt;/b&gt;&lt;p&gt;
package type TQ</description>
</package>
<package name="PULSE_BH">
</package>
<package name="HC73">
</package>
<package name="MNR35">
</package>
<package name="SOT223-6">
<description>SOT223-6 ass found in TPS736xx data sheet</description>
</package>
<package name="QFN24_4X4">
</package>
<package name="NV08C-CSM">
</package>
<package name="JACK2.5_SJ-2523">
</package>
<package name="BA2023-ND">
<description>Footprint taken from BA2032/datasheet.pdf  6/27/08

Memory Protection Devices, Inc</description>
</package>
<package name="MOLEX_MCX_V">
</package>
<package name="0603">
</package>
<package name="TSSOP20">
</package>
<package name="TSSOP8">
</package>
<package name="TSSOP16">
</package>
<package name="SOT223">
</package>
<package name="SOT143">
</package>
<package name="DB9_TE">
<description>TE Connectivity SUB-D male 9pin, right angle, 8.08mm 
1734351-1</description>
</package>
<package name="CORTEX_SWD_TH_2X5">
</package>
<package name="HSEC8-130-01-X-DV-A">
<description>0.8MM PITCH HIGH SPEED ASSEMBLY, 60PINS</description>
</package>
</packages>
<symbols>
<symbol name="NCN8025">
<pin name="VDDP" direction="pwr"/>
<pin name="VSEL0" direction="in"/>
<pin name="VSEL1" direction="in"/>
<pin name="/CMDVCC" direction="in"/>
<pin name="/INT" direction="out"/>
<pin name="CLKDIV1" direction="in"/>
<pin name="CLKDIV2"/>
<pin name="CLKIN"/>
<pin name="RSTIN" direction="in"/>
<pin name="IO_UC"/>
<pin name="GND2" direction="pwr"/>
<pin name="C_RST" direction="out"/>
<pin name="C_IO"/>
<pin name="C_CLK" direction="out"/>
<pin name="/PRES" direction="in"/>
<pin name="C_VCC" direction="in"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="NC8025A">
<pin name="GND" direction="pwr"/>
<pin name="VDDP" direction="pwr"/>
<pin name="PORADJ" direction="in"/>
<pin name="VSEL0" direction="in"/>
<pin name="VSEL1" direction="in"/>
<pin name="/CMDVCC" direction="in"/>
<pin name="/INT" direction="out"/>
<pin name="CLKDIV1" direction="in"/>
<pin name="CLKDIV2"/>
<pin name="CLKIN"/>
<pin name="RSTIN" direction="in"/>
<pin name="IO_UC"/>
<pin name="AUX1_UC"/>
<pin name="AUX2_UC"/>
<pin name="GND2" direction="pwr"/>
<pin name="C_RST" direction="out"/>
<pin name="C_IO"/>
<pin name="C_AUX1"/>
<pin name="GND3"/>
<pin name="C_AUX2"/>
<pin name="C_CLK" direction="out"/>
<pin name="PRES" direction="in"/>
<pin name="/PRES" direction="in"/>
<pin name="C_VCC" direction="in"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="SIM">
<pin name="VCC" direction="pwr"/>
<pin name="RST" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="AUX1"/>
<pin name="AUX2"/>
<pin name="I/O"/>
<pin name="VPP" direction="pwr"/>
<pin name="GND"/>
</symbol>
<symbol name="SIM_SW_NO">
<pin name="0@A" direction="pas"/>
<pin name="1@A" direction="pas"/>
</symbol>
<symbol name="CON_CORTEX_DBG">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="KEY"/>
<pin name="GNDDETECT"/>
<pin name="/RESET"/>
<pin name="NC"/>
<pin name="SWO"/>
<pin name="SWDCLK"/>
<pin name="SWDIO"/>
</symbol>
<symbol name="IDT82V2081_TDM">
<pin name="LOS" direction="out"/>
<pin name="RCLK" direction="out"/>
<pin name="RD/RDP" direction="out"/>
<pin name="CV/RDN" direction="out"/>
<pin name="TCLK" direction="in"/>
<pin name="TD/TDP" direction="in"/>
<pin name="TDN" direction="in"/>
</symbol>
<symbol name="IDT82V2081_LINE">
<pin name="RTIP" direction="in"/>
<pin name="RRING" direction="in"/>
<pin name="TTIP" direction="out"/>
<pin name="TRING" direction="out"/>
</symbol>
<symbol name="IDT82V2081_SERIAL">
<pin name="!INT" direction="out"/>
<pin name="!CS" direction="in"/>
<pin name="SDO/!ACK/RDY" direction="out"/>
<pin name="SCLK/ALE/AS" direction="in"/>
<pin name="!RD/DS/SCLKE" direction="in"/>
<pin name="SDI/WR/RW" direction="in"/>
</symbol>
<symbol name="IDT82V2081_PINCTRL">
<pin name="MODE0" direction="in"/>
<pin name="MODE1" direction="in"/>
<pin name="PULS0/AD4" direction="in"/>
<pin name="PULS1/AD5" direction="in"/>
<pin name="PULS2/AD6" direction="in"/>
<pin name="PULS3/AD7" direction="in"/>
<pin name="EQ/AD3" direction="in"/>
<pin name="RPD/AD2" direction="in"/>
<pin name="PATT1/AD1" direction="in"/>
<pin name="PATT0/AD0" direction="in"/>
<pin name="JA0" direction="in"/>
<pin name="JA1" direction="in"/>
<pin name="THZ" direction="in"/>
<pin name="!RST" direction="in"/>
<pin name="RCLKE" direction="in"/>
</symbol>
<symbol name="IDT82V2081_V">
<pin name="GNDT" direction="pwr"/>
<pin name="GNDA" direction="pwr"/>
<pin name="VDDD" direction="pwr"/>
<pin name="VDDT" direction="pwr"/>
<pin name="REF" direction="in"/>
<pin name="GNDD" direction="pwr"/>
<pin name="VDDA" direction="pwr"/>
<pin name="VDDIO" direction="pwr"/>
<pin name="GNDIO" direction="pwr"/>
</symbol>
<symbol name="IDT82V2081_MISC">
<pin name="MCLK" direction="pwr"/>
<pin name="IC0" direction="nc"/>
<pin name="IC1" direction="nc"/>
</symbol>
<symbol name="E1_MAGNETICS">
<pin name="P$1"/>
<pin name="P$2"/>
<pin name="P$3"/>
<pin name="P$4"/>
<pin name="P$5"/>
<pin name="P$6"/>
</symbol>
<symbol name="OSCILLATOR">
<pin name="E/D" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="RESNET8">
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="C" direction="pas"/>
<pin name="D" direction="pas"/>
</symbol>
<symbol name="LDO_EN">
<pin name="IN" direction="in"/>
<pin name="OUT" direction="pas"/>
<pin name="EN" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="NR" direction="pas"/>
<pin name="GND1" direction="pwr"/>
</symbol>
<symbol name="NV08C-CSM">
<pin name="ANT_GND1"/>
<pin name="ANT_IN" direction="in"/>
<pin name="ANT_GND2"/>
<pin name="GPIO0"/>
<pin name="GPIO1"/>
<pin name="GPIO2"/>
<pin name="GPIO3"/>
<pin name="GPIO4"/>
<pin name="GPIO5"/>
<pin name="GPIO6"/>
<pin name="GPIO7"/>
<pin name="RX1" direction="in"/>
<pin name="TX1" direction="out"/>
<pin name="RX2" direction="in"/>
<pin name="TX2" direction="out"/>
<pin name="VIN_A" direction="pwr"/>
<pin name="RF_SHDN" direction="out"/>
<pin name="VBAT" direction="in"/>
<pin name="VIN_D" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="GND1"/>
<pin name="GND2"/>
<pin name="GND3"/>
<pin name="GND4"/>
<pin name="GND5"/>
<pin name="GND6"/>
<pin name="GND7"/>
<pin name="GND8"/>
<pin name="GND9"/>
<pin name="GND10"/>
<pin name="GND11"/>
<pin name="GND12"/>
<pin name="!RES" direction="in"/>
<pin name="GND13"/>
<pin name="GND14"/>
</symbol>
<symbol name="JACK2.5STEREO">
<pin name="RING" direction="pas"/>
<pin name="TIP" direction="pas"/>
<pin name="MIDDLE" direction="pas"/>
</symbol>
<symbol name="BATTERY">
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
<pin name="+@1" direction="pas"/>
</symbol>
<symbol name="COAX_FGND">
<pin name="1" direction="pas"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="GND">
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="L-EU">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="SP3203E">
<pin name="C1+"/>
<pin name="C1-"/>
<pin name="C2+"/>
<pin name="C2-"/>
<pin name="T1IN" direction="in"/>
<pin name="T2IN" direction="in"/>
<pin name="R1OUT" direction="out"/>
<pin name="R2OUT" direction="out"/>
<pin name="V+"/>
<pin name="V-"/>
<pin name="T1OUT" direction="out"/>
<pin name="T2OUT" direction="out"/>
<pin name="R1IN" direction="in"/>
<pin name="R2IN" direction="in"/>
<pin name="VL" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="!SHDN" direction="in"/>
<pin name="GND"/>
<pin name="T3IN" direction="in"/>
<pin name="T3OUT" direction="out"/>
</symbol>
<symbol name="74*2T45">
<pin name="1A"/>
<pin name="2A"/>
<pin name="2B"/>
<pin name="1B"/>
<pin name="DIR" direction="in"/>
<pin name="VCC_B" direction="pwr"/>
<pin name="VCC_A"/>
<pin name="GND" direction="pas"/>
</symbol>
<symbol name="74*4T245">
<pin name="1A1"/>
<pin name="1A2"/>
<pin name="1B2"/>
<pin name="1B1"/>
<pin name="1DIR" direction="in"/>
<pin name="VCC_B" direction="pwr"/>
<pin name="VCC_A"/>
<pin name="GND" direction="pas"/>
<pin name="2A1"/>
<pin name="2A2"/>
<pin name="2B2"/>
<pin name="2B1"/>
<pin name="2DIR" direction="in"/>
<pin name="GND1" direction="pas"/>
<pin name="!1OE" direction="in"/>
<pin name="!2OE" direction="in"/>
</symbol>
<symbol name="LDO">
<pin name="IN" direction="in"/>
<pin name="OUT" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="OUT1" direction="pas"/>
</symbol>
<symbol name="DIODE_ARRAY3">
<pin name="A" direction="pas"/>
<pin name="K" direction="pas"/>
<pin name="K1" direction="pas"/>
<pin name="K2" direction="pas"/>
</symbol>
<symbol name="SUBD9M">
<pin name="1" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="G1" direction="pas"/>
<pin name="G2" direction="pas"/>
</symbol>
<symbol name="SYSMOBTS_PROD_PWR">
<pin name="5VDC_1" direction="sup"/>
<pin name="5VDC_2" direction="sup"/>
<pin name="3V3DC_1" direction="sup"/>
<pin name="3V3DC_2" direction="sup"/>
<pin name="1V8DC_1" direction="sup"/>
<pin name="1V8DC_2" direction="sup"/>
<pin name="1V2DC_1" direction="sup"/>
<pin name="1V2DC_2" direction="sup"/>
<pin name="1V2CORE_1" direction="sup"/>
<pin name="1V2CORE_2" direction="sup"/>
<pin name="GND5" direction="sup"/>
<pin name="GND4" direction="sup"/>
<pin name="GND3" direction="sup"/>
<pin name="GND2" direction="sup"/>
<pin name="GND1" direction="sup"/>
</symbol>
<symbol name="SYSMOBTS_PROD_SPI">
<pin name="SPICLK" direction="out"/>
<pin name="SPIEN1" direction="out"/>
<pin name="SPIEN0" direction="out"/>
<pin name="SPIDI" direction="in"/>
<pin name="SPIDO" direction="out"/>
<pin name="GND1" direction="pas"/>
<pin name="GND2" direction="pas"/>
<pin name="DSP_BTSEL1" direction="in"/>
<pin name="DSP_BTSEL0" direction="in"/>
<pin name="UART_TX0" direction="out"/>
<pin name="UART_RX0" direction="in"/>
<pin name="I2C_SDA"/>
<pin name="I2C_SCL"/>
</symbol>
<symbol name="SYSMOBTS_PROD_FPGA_JTAG">
<pin name="FPGA_TDI" direction="in"/>
<pin name="FPGA_TDO" direction="out"/>
<pin name="FPGA_TCK" direction="in"/>
<pin name="FPGA_TMS" direction="in"/>
<pin name="FPGA_GND" direction="pas"/>
</symbol>
<symbol name="SYSMOBTS_PROD_DSP_JTAG">
<pin name="DSP_TMS" direction="in"/>
<pin name="DSP_TRST" direction="in"/>
<pin name="DSP_TDI" direction="in"/>
<pin name="DSP_TDO" direction="out"/>
<pin name="DSP_RTCK" direction="out"/>
<pin name="DSP_TCK" direction="in"/>
<pin name="DSP_EMU0" direction="sup"/>
<pin name="DSP_EMU1" direction="sup"/>
<pin name="DSP_GND" direction="sup"/>
</symbol>
<symbol name="SYSMOBTS_CPLD_JTAG">
<pin name="CPLD_TCK" direction="sup"/>
<pin name="CPLD_TDI" direction="sup"/>
<pin name="CPLD_TDO" direction="sup"/>
<pin name="CPLD_TMS" direction="sup"/>
<pin name="CPLD_GND" direction="sup"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="NCN8025">
<gates>
<gate name="G$1" symbol="NCN8025"/>
</gates>
<devices>
<device name="QFN16" package="QFN16_3X3">
<connects>
<connect gate="G$1" pin="/CMDVCC" pad="8"/>
<connect gate="G$1" pin="/INT" pad="11"/>
<connect gate="G$1" pin="/PRES" pad="3"/>
<connect gate="G$1" pin="CLKDIV1" pad="14"/>
<connect gate="G$1" pin="CLKDIV2" pad="15"/>
<connect gate="G$1" pin="CLKIN" pad="12"/>
<connect gate="G$1" pin="C_CLK" pad="5"/>
<connect gate="G$1" pin="C_IO" pad="4"/>
<connect gate="G$1" pin="C_RST" pad="6"/>
<connect gate="G$1" pin="C_VCC" pad="7"/>
<connect gate="G$1" pin="GND2" pad="EXP"/>
<connect gate="G$1" pin="IO_UC" pad="13"/>
<connect gate="G$1" pin="RSTIN" pad="9"/>
<connect gate="G$1" pin="VDD" pad="10"/>
<connect gate="G$1" pin="VDDP" pad="2"/>
<connect gate="G$1" pin="VSEL0" pad="1"/>
<connect gate="G$1" pin="VSEL1" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="QFN24" package="QFN24_4X4">
<connects>
<connect gate="G$1" pin="/CMDVCC" pad="12"/>
<connect gate="G$1" pin="/INT" pad="17"/>
<connect gate="G$1" pin="/PRES" pad="3"/>
<connect gate="G$1" pin="CLKDIV1" pad="22"/>
<connect gate="G$1" pin="CLKDIV2" pad="23"/>
<connect gate="G$1" pin="CLKIN" pad="18"/>
<connect gate="G$1" pin="C_CLK" pad="9"/>
<connect gate="G$1" pin="C_IO" pad="5"/>
<connect gate="G$1" pin="C_RST" pad="10"/>
<connect gate="G$1" pin="C_VCC" pad="11"/>
<connect gate="G$1" pin="GND2" pad="25"/>
<connect gate="G$1" pin="IO_UC" pad="19"/>
<connect gate="G$1" pin="RSTIN" pad="14"/>
<connect gate="G$1" pin="VDD" pad="15"/>
<connect gate="G$1" pin="VDDP" pad="2"/>
<connect gate="G$1" pin="VSEL0" pad="1"/>
<connect gate="G$1" pin="VSEL1" pad="24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AMPHENOL_SIM">
<gates>
<gate name="G$1" symbol="SIM"/>
<gate name="G$2" symbol="SIM_SW_NO"/>
</gates>
<devices>
<device name="" package="AMPHENOL_SIM">
<connects>
<connect gate="G$1" pin="AUX1" pad="C7"/>
<connect gate="G$1" pin="AUX2" pad="C8"/>
<connect gate="G$1" pin="CLK" pad="CLK"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="I/O" pad="IO"/>
<connect gate="G$1" pin="RST" pad="RST"/>
<connect gate="G$1" pin="VCC" pad="VCC_SIM"/>
<connect gate="G$1" pin="VPP" pad="VPP"/>
<connect gate="G$2" pin="0@A" pad="SW1"/>
<connect gate="G$2" pin="1@A" pad="SW2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CON_CORTEX_DBG">
<description>Connectors for the ARM CORTEX SWD</description>
<gates>
<gate name="G$1" symbol="CON_CORTEX_DBG"/>
</gates>
<devices>
<device name="" package="FTSH-105-01-XXX-DV-K">
<connects>
<connect gate="G$1" pin="/RESET" pad="10"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="GND2" pad="5"/>
<connect gate="G$1" pin="GNDDETECT" pad="9"/>
<connect gate="G$1" pin="KEY" pad="7"/>
<connect gate="G$1" pin="NC" pad="8"/>
<connect gate="G$1" pin="SWDCLK" pad="4"/>
<connect gate="G$1" pin="SWDIO" pad="2"/>
<connect gate="G$1" pin="SWO" pad="6"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TH" package="CORTEX_SWD_TH_2X5">
<connects>
<connect gate="G$1" pin="/RESET" pad="10"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="GND2" pad="5"/>
<connect gate="G$1" pin="GNDDETECT" pad="9"/>
<connect gate="G$1" pin="KEY" pad="7"/>
<connect gate="G$1" pin="NC" pad="8"/>
<connect gate="G$1" pin="SWDCLK" pad="4"/>
<connect gate="G$1" pin="SWDIO" pad="2"/>
<connect gate="G$1" pin="SWO" pad="6"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IDT82V2081">
<gates>
<gate name="G$1" symbol="IDT82V2081_TDM"/>
<gate name="G$2" symbol="IDT82V2081_LINE"/>
<gate name="G$3" symbol="IDT82V2081_SERIAL"/>
<gate name="G$4" symbol="IDT82V2081_PINCTRL"/>
<gate name="G$5" symbol="IDT82V2081_V"/>
<gate name="G$6" symbol="IDT82V2081_MISC"/>
</gates>
<devices>
<device name="" package="TQFP44">
<connects>
<connect gate="G$1" pin="CV/RDN" pad="6"/>
<connect gate="G$1" pin="LOS" pad="7"/>
<connect gate="G$1" pin="RCLK" pad="4"/>
<connect gate="G$1" pin="RD/RDP" pad="5"/>
<connect gate="G$1" pin="TCLK" pad="1"/>
<connect gate="G$1" pin="TD/TDP" pad="2"/>
<connect gate="G$1" pin="TDN" pad="3"/>
<connect gate="G$2" pin="RRING" pad="40"/>
<connect gate="G$2" pin="RTIP" pad="41"/>
<connect gate="G$2" pin="TRING" pad="36"/>
<connect gate="G$2" pin="TTIP" pad="37"/>
<connect gate="G$3" pin="!CS" pad="21"/>
<connect gate="G$3" pin="!INT" pad="20"/>
<connect gate="G$3" pin="!RD/DS/SCLKE" pad="22"/>
<connect gate="G$3" pin="SCLK/ALE/AS" pad="25"/>
<connect gate="G$3" pin="SDI/WR/RW" pad="24"/>
<connect gate="G$3" pin="SDO/!ACK/RDY" pad="23"/>
<connect gate="G$4" pin="!RST" pad="12"/>
<connect gate="G$4" pin="EQ/AD3" pad="29"/>
<connect gate="G$4" pin="JA0" pad="14"/>
<connect gate="G$4" pin="JA1" pad="15"/>
<connect gate="G$4" pin="MODE0" pad="16"/>
<connect gate="G$4" pin="MODE1" pad="17"/>
<connect gate="G$4" pin="PATT0/AD0" pad="26"/>
<connect gate="G$4" pin="PATT1/AD1" pad="27"/>
<connect gate="G$4" pin="PULS0/AD4" pad="30"/>
<connect gate="G$4" pin="PULS1/AD5" pad="31"/>
<connect gate="G$4" pin="PULS2/AD6" pad="32"/>
<connect gate="G$4" pin="PULS3/AD7" pad="33"/>
<connect gate="G$4" pin="RCLKE" pad="11"/>
<connect gate="G$4" pin="RPD/AD2" pad="28"/>
<connect gate="G$4" pin="THZ" pad="13"/>
<connect gate="G$5" pin="GNDA" pad="39"/>
<connect gate="G$5" pin="GNDD" pad="10"/>
<connect gate="G$5" pin="GNDIO" pad="18"/>
<connect gate="G$5" pin="GNDT" pad="38"/>
<connect gate="G$5" pin="REF" pad="43"/>
<connect gate="G$5" pin="VDDA" pad="42"/>
<connect gate="G$5" pin="VDDD" pad="8"/>
<connect gate="G$5" pin="VDDIO" pad="19"/>
<connect gate="G$5" pin="VDDT" pad="35"/>
<connect gate="G$6" pin="IC0" pad="44"/>
<connect gate="G$6" pin="IC1" pad="34"/>
<connect gate="G$6" pin="MCLK" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PULSE_T1094NL">
<gates>
<gate name="1:1" symbol="E1_MAGNETICS"/>
<gate name="2:1" symbol="E1_MAGNETICS"/>
</gates>
<devices>
<device name="" package="PULSE_BH">
<connects>
<connect gate="1:1" pin="P$1" pad="P$1"/>
<connect gate="1:1" pin="P$2" pad="P$2"/>
<connect gate="1:1" pin="P$3" pad="P$3"/>
<connect gate="1:1" pin="P$4" pad="P$16"/>
<connect gate="1:1" pin="P$5" pad="P$15"/>
<connect gate="1:1" pin="P$6" pad="P$14"/>
<connect gate="2:1" pin="P$1" pad="P$6"/>
<connect gate="2:1" pin="P$2" pad="P$7"/>
<connect gate="2:1" pin="P$3" pad="P$8"/>
<connect gate="2:1" pin="P$4" pad="P$11"/>
<connect gate="2:1" pin="P$5" pad="P$10"/>
<connect gate="2:1" pin="P$6" pad="P$9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FOX_FXO-HC73">
<gates>
<gate name="G$1" symbol="OSCILLATOR"/>
</gates>
<devices>
<device name="" package="HC73">
<connects>
<connect gate="G$1" pin="E/D" pad="P$1"/>
<connect gate="G$1" pin="GND" pad="P$2"/>
<connect gate="G$1" pin="OUT" pad="P$3"/>
<connect gate="G$1" pin="VCC" pad="P$4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MNR">
<description>Rohm 8-element Chip Resistor Network

MNR35 (1206x5 size)</description>
<gates>
<gate name="G$1" symbol="RESNET8"/>
</gates>
<devices>
<device name="" package="MNR35">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="9"/>
<connect gate="G$1" pin="6" pad="8"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="6"/>
<connect gate="G$1" pin="C" pad="5"/>
<connect gate="G$1" pin="D" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TPS736XX">
<description>TI Cap-Free NMOS 400mA LDO</description>
<gates>
<gate name="G$1" symbol="LDO_EN"/>
</gates>
<devices>
<device name="" package="SOT223-6">
<connects>
<connect gate="G$1" pin="EN" pad="5"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="GND1" pad="6"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="NR" pad="4"/>
<connect gate="G$1" pin="OUT" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCN8025A">
<gates>
<gate name="G$1" symbol="NC8025A"/>
</gates>
<devices>
<device name="" package="QFN24_4X4">
<connects>
<connect gate="G$1" pin="/CMDVCC" pad="12"/>
<connect gate="G$1" pin="/INT" pad="17"/>
<connect gate="G$1" pin="/PRES" pad="3"/>
<connect gate="G$1" pin="AUX1_UC" pad="20"/>
<connect gate="G$1" pin="AUX2_UC" pad="21"/>
<connect gate="G$1" pin="CLKDIV1" pad="22"/>
<connect gate="G$1" pin="CLKDIV2" pad="23"/>
<connect gate="G$1" pin="CLKIN" pad="18"/>
<connect gate="G$1" pin="C_AUX1" pad="7"/>
<connect gate="G$1" pin="C_AUX2" pad="6"/>
<connect gate="G$1" pin="C_CLK" pad="9"/>
<connect gate="G$1" pin="C_IO" pad="5"/>
<connect gate="G$1" pin="C_RST" pad="10"/>
<connect gate="G$1" pin="C_VCC" pad="11"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="GND2" pad="16"/>
<connect gate="G$1" pin="GND3" pad="25"/>
<connect gate="G$1" pin="IO_UC" pad="19"/>
<connect gate="G$1" pin="PORADJ" pad="13"/>
<connect gate="G$1" pin="PRES" pad="4"/>
<connect gate="G$1" pin="RSTIN" pad="14"/>
<connect gate="G$1" pin="VDD" pad="15"/>
<connect gate="G$1" pin="VDDP" pad="2"/>
<connect gate="G$1" pin="VSEL0" pad="1"/>
<connect gate="G$1" pin="VSEL1" pad="24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NV08C-CSM">
<gates>
<gate name="G$1" symbol="NV08C-CSM"/>
</gates>
<devices>
<device name="" package="NV08C-CSM">
<connects>
<connect gate="G$1" pin="!RES" pad="25"/>
<connect gate="G$1" pin="ANT_GND1" pad="14"/>
<connect gate="G$1" pin="ANT_GND2" pad="16"/>
<connect gate="G$1" pin="ANT_IN" pad="15"/>
<connect gate="G$1" pin="GND1" pad="3"/>
<connect gate="G$1" pin="GND10" pad="22"/>
<connect gate="G$1" pin="GND11" pad="24"/>
<connect gate="G$1" pin="GND12" pad="27"/>
<connect gate="G$1" pin="GND13" pad="29"/>
<connect gate="G$1" pin="GND14" pad="34"/>
<connect gate="G$1" pin="GND2" pad="9"/>
<connect gate="G$1" pin="GND3" pad="10"/>
<connect gate="G$1" pin="GND4" pad="11"/>
<connect gate="G$1" pin="GND5" pad="12"/>
<connect gate="G$1" pin="GND6" pad="13"/>
<connect gate="G$1" pin="GND7" pad="17"/>
<connect gate="G$1" pin="GND8" pad="18"/>
<connect gate="G$1" pin="GND9" pad="19"/>
<connect gate="G$1" pin="GPIO0" pad="20"/>
<connect gate="G$1" pin="GPIO1" pad="2"/>
<connect gate="G$1" pin="GPIO2" pad="1"/>
<connect gate="G$1" pin="GPIO3" pad="6"/>
<connect gate="G$1" pin="GPIO4" pad="7"/>
<connect gate="G$1" pin="GPIO5" pad="4"/>
<connect gate="G$1" pin="GPIO6" pad="35"/>
<connect gate="G$1" pin="GPIO7" pad="5"/>
<connect gate="G$1" pin="RF_SHDN" pad="21"/>
<connect gate="G$1" pin="RX1" pad="33"/>
<connect gate="G$1" pin="RX2" pad="30"/>
<connect gate="G$1" pin="TX1" pad="32"/>
<connect gate="G$1" pin="TX2" pad="31"/>
<connect gate="G$1" pin="VBAT" pad="23"/>
<connect gate="G$1" pin="VCCIO" pad="28"/>
<connect gate="G$1" pin="VIN_A" pad="8"/>
<connect gate="G$1" pin="VIN_D" pad="26"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JACK2.5_SJ-2523">
<description>CUI Inc. SJ-2523-SMT</description>
<gates>
<gate name="G$1" symbol="JACK2.5STEREO"/>
</gates>
<devices>
<device name="" package="JACK2.5_SJ-2523">
<connects>
<connect gate="G$1" pin="MIDDLE" pad="3"/>
<connect gate="G$1" pin="RING" pad="1"/>
<connect gate="G$1" pin="TIP" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BA2032">
<gates>
<gate name="G$1" symbol="BATTERY"/>
</gates>
<devices>
<device name="" package="BA2023-ND">
<connects>
<connect gate="G$1" pin="+" pad="P$2"/>
<connect gate="G$1" pin="+@1" pad="P$1"/>
<connect gate="G$1" pin="-" pad="P$3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOLEX_MCX_V">
<description>Molex 73366-0061 / Digi-Key WM5441-ND

MCX straight vertical through-hold 50Ohms</description>
<gates>
<gate name="G$1" symbol="COAX_FGND"/>
<gate name="G$2" symbol="GND"/>
<gate name="G$3" symbol="GND"/>
<gate name="G$4" symbol="GND"/>
</gates>
<devices>
<device name="" package="MOLEX_MCX_V">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="GND" pad="P$2"/>
<connect gate="G$2" pin="GND" pad="P$3"/>
<connect gate="G$3" pin="GND" pad="P$4"/>
<connect gate="G$4" pin="GND" pad="P$5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="L-EU0603">
<gates>
<gate name="G$1" symbol="L-EU"/>
</gates>
<devices>
<device name="" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SP3203E">
<description>Exar SP3203E RS232 transceiver with variable CMOS Voltage

Taken from SP3203E_100_120810</description>
<gates>
<gate name="G$1" symbol="SP3203E"/>
</gates>
<devices>
<device name="" package="TSSOP20">
<connects>
<connect gate="G$1" pin="!SHDN" pad="20"/>
<connect gate="G$1" pin="C1+" pad="1"/>
<connect gate="G$1" pin="C1-" pad="3"/>
<connect gate="G$1" pin="C2+" pad="4"/>
<connect gate="G$1" pin="C2-" pad="5"/>
<connect gate="G$1" pin="GND" pad="18"/>
<connect gate="G$1" pin="R1IN" pad="14"/>
<connect gate="G$1" pin="R1OUT" pad="11"/>
<connect gate="G$1" pin="R2IN" pad="13"/>
<connect gate="G$1" pin="R2OUT" pad="10"/>
<connect gate="G$1" pin="T1IN" pad="7"/>
<connect gate="G$1" pin="T1OUT" pad="17"/>
<connect gate="G$1" pin="T2IN" pad="8"/>
<connect gate="G$1" pin="T2OUT" pad="16"/>
<connect gate="G$1" pin="T3IN" pad="9"/>
<connect gate="G$1" pin="T3OUT" pad="15"/>
<connect gate="G$1" pin="V+" pad="2"/>
<connect gate="G$1" pin="V-" pad="6"/>
<connect gate="G$1" pin="VCC" pad="19"/>
<connect gate="G$1" pin="VL" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AVC2T45">
<description>NXP 74AVC2T45 DUAL-BIT, DUAL-SUPPLY VOLTAGE LEVEL TRANSLATOR/TRANSCEIVER; TRI-STATE</description>
<gates>
<gate name="G$1" symbol="74*2T45"/>
</gates>
<devices>
<device name="" package="TSSOP8">
<connects>
<connect gate="G$1" pin="1A" pad="2"/>
<connect gate="G$1" pin="1B" pad="7"/>
<connect gate="G$1" pin="2A" pad="3"/>
<connect gate="G$1" pin="2B" pad="6"/>
<connect gate="G$1" pin="DIR" pad="5"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VCC_A" pad="1"/>
<connect gate="G$1" pin="VCC_B" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SN74AVC4T245">
<gates>
<gate name="G$1" symbol="74*4T245"/>
</gates>
<devices>
<device name="" package="TSSOP16">
<connects>
<connect gate="G$1" pin="!1OE" pad="15"/>
<connect gate="G$1" pin="!2OE" pad="14"/>
<connect gate="G$1" pin="1A1" pad="4"/>
<connect gate="G$1" pin="1A2" pad="5"/>
<connect gate="G$1" pin="1B1" pad="13"/>
<connect gate="G$1" pin="1B2" pad="12"/>
<connect gate="G$1" pin="1DIR" pad="2"/>
<connect gate="G$1" pin="2A1" pad="6"/>
<connect gate="G$1" pin="2A2" pad="7"/>
<connect gate="G$1" pin="2B1" pad="11"/>
<connect gate="G$1" pin="2B2" pad="10"/>
<connect gate="G$1" pin="2DIR" pad="3"/>
<connect gate="G$1" pin="GND" pad="9"/>
<connect gate="G$1" pin="GND1" pad="8"/>
<connect gate="G$1" pin="VCC_A" pad="1"/>
<connect gate="G$1" pin="VCC_B" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TPS732XX">
<description>TI TPS732xx Cao-free NMOS 250mA LDO</description>
<gates>
<gate name="G$1" symbol="LDO_EN"/>
</gates>
<devices>
<device name="" package="SOT223-6">
<connects>
<connect gate="G$1" pin="EN" pad="5"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="GND1" pad="6"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="NR" pad="4"/>
<connect gate="G$1" pin="OUT" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TLV1117">
<gates>
<gate name="G$1" symbol="LDO"/>
</gates>
<devices>
<device name="" package="SOT223">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="OUT" pad="2"/>
<connect gate="G$1" pin="OUT1" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SP0503BAHT">
<gates>
<gate name="G$1" symbol="DIODE_ARRAY3"/>
</gates>
<devices>
<device name="" package="SOT143">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="K" pad="2"/>
<connect gate="G$1" pin="K1" pad="3"/>
<connect gate="G$1" pin="K2" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TE_SUBD9M">
<description>TE connectivity 1734351-1</description>
<gates>
<gate name="G$1" symbol="SUBD9M"/>
</gates>
<devices>
<device name="" package="DB9_TE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="G1" pad="G1"/>
<connect gate="G$1" pin="G2" pad="G2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SYSMOBTS_PROD">
<description>SysmoBTS Production connector (2x30pin)</description>
<gates>
<gate name="G$1" symbol="SYSMOBTS_PROD_PWR"/>
<gate name="G$2" symbol="SYSMOBTS_PROD_SPI"/>
<gate name="G$3" symbol="SYSMOBTS_PROD_FPGA_JTAG"/>
<gate name="G$4" symbol="SYSMOBTS_PROD_DSP_JTAG"/>
<gate name="G$5" symbol="SYSMOBTS_CPLD_JTAG"/>
</gates>
<devices>
<device name="" package="HSEC8-130-01-X-DV-A">
<connects>
<connect gate="G$1" pin="1V2CORE_1" pad="A13"/>
<connect gate="G$1" pin="1V2CORE_2" pad="A14"/>
<connect gate="G$1" pin="1V2DC_1" pad="A10"/>
<connect gate="G$1" pin="1V2DC_2" pad="A11"/>
<connect gate="G$1" pin="1V8DC_1" pad="A7"/>
<connect gate="G$1" pin="1V8DC_2" pad="A8"/>
<connect gate="G$1" pin="3V3DC_1" pad="A4"/>
<connect gate="G$1" pin="3V3DC_2" pad="A5"/>
<connect gate="G$1" pin="5VDC_1" pad="A1"/>
<connect gate="G$1" pin="5VDC_2" pad="A2"/>
<connect gate="G$1" pin="GND1" pad="A16"/>
<connect gate="G$1" pin="GND2" pad="A17"/>
<connect gate="G$1" pin="GND3" pad="A18"/>
<connect gate="G$1" pin="GND4" pad="A19"/>
<connect gate="G$1" pin="GND5" pad="A20"/>
<connect gate="G$2" pin="DSP_BTSEL0" pad="B2"/>
<connect gate="G$2" pin="DSP_BTSEL1" pad="B1"/>
<connect gate="G$2" pin="GND1" pad="B3"/>
<connect gate="G$2" pin="GND2" pad="B6"/>
<connect gate="G$2" pin="I2C_SCL" pad="B7"/>
<connect gate="G$2" pin="I2C_SDA" pad="B8"/>
<connect gate="G$2" pin="SPICLK" pad="A25"/>
<connect gate="G$2" pin="SPIDI" pad="A28"/>
<connect gate="G$2" pin="SPIDO" pad="A29"/>
<connect gate="G$2" pin="SPIEN0" pad="A27"/>
<connect gate="G$2" pin="SPIEN1" pad="A26"/>
<connect gate="G$2" pin="UART_RX0" pad="B5"/>
<connect gate="G$2" pin="UART_TX0" pad="B4"/>
<connect gate="G$3" pin="FPGA_GND" pad="B14"/>
<connect gate="G$3" pin="FPGA_TCK" pad="B12"/>
<connect gate="G$3" pin="FPGA_TDI" pad="B10"/>
<connect gate="G$3" pin="FPGA_TDO" pad="B11"/>
<connect gate="G$3" pin="FPGA_TMS" pad="B13"/>
<connect gate="G$4" pin="DSP_EMU0" pad="B21"/>
<connect gate="G$4" pin="DSP_EMU1" pad="B22"/>
<connect gate="G$4" pin="DSP_GND" pad="B23"/>
<connect gate="G$4" pin="DSP_RTCK" pad="B19"/>
<connect gate="G$4" pin="DSP_TCK" pad="B20"/>
<connect gate="G$4" pin="DSP_TDI" pad="B17"/>
<connect gate="G$4" pin="DSP_TDO" pad="B18"/>
<connect gate="G$4" pin="DSP_TMS" pad="B15"/>
<connect gate="G$4" pin="DSP_TRST" pad="B16"/>
<connect gate="G$5" pin="CPLD_GND" pad="B28"/>
<connect gate="G$5" pin="CPLD_TCK" pad="B24"/>
<connect gate="G$5" pin="CPLD_TDI" pad="B25"/>
<connect gate="G$5" pin="CPLD_TDO" pad="B26"/>
<connect gate="G$5" pin="CPLD_TMS" pad="B27"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
