<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="50" y2="0" width="0" layer="20"/>
<wire x1="50" y1="0" x2="50" y2="100" width="0" layer="20"/>
<wire x1="50" y1="100" x2="0" y2="100" width="0" layer="20"/>
<wire x1="0" y1="100" x2="0" y2="0" width="0" layer="20"/>
<text>osmo-clock-converter
(C) 2019 by
Harald Welte
Mfg: sysmocom GmbH
OSHW / CC-BY-SA</text>
<text>osmo-clock-converter
(C) 2019 by
Harald Welte
Mfg: sysmocom GmbH
OSHW / CC-BY-SA</text>
<text>&gt;REVISION</text>
<text>Version:</text>
</plain>
<libraries>
<library name="rc-sysmocom">
<packages>
<package name="_0603">
<description>&lt;b&gt;0603&lt;/b&gt;</description>
</package>
<package name="_0805">
<description>&lt;b&gt;0805&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="laforge">
<description>&lt;b&gt;PCB Matrix Packages&lt;/b&gt;&lt;p&gt;</description>
<packages>
<package name="0603">
</package>
<package name="1X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="HRS_UFL">
<description>&lt;b&gt;Hirose U.FL SMT&lt;/b&gt;</description>
</package>
<package name="SMA-F-S-TH">
</package>
</packages>
</library>
<library name="diodes-sysmocom">
<packages>
<package name="SMADIODE">
<description>&lt;b&gt;SMA Surface Mount Diode&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="littlefuse">
<packages>
<package name="1206L">
<description>From Littelfuse POLY-FUSE 1206L data sheet</description>
</package>
</packages>
</library>
<library name="jumper">
<description>&lt;b&gt;Jumpers&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="JP2">
<description>&lt;b&gt;JUMPER&lt;/b&gt;</description>
</package>
<package name="JP1">
<description>&lt;b&gt;JUMPER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X04">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="Wurth_Elektronik_Electromechanic_DC_Power_Jack_Connectors_rev15c">
<description>&lt;BR&gt;Wurth Elektronik - DC Power Jack Connectors&lt;br&gt;&lt;Hr&gt;
&lt;BR&gt;&lt;BR&gt; 
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-405&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/eagle"&gt;http://www.we-online.com/eagle &lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither CadSoft nor WE-eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;&lt;BR&gt;&lt;br&gt;
&lt;hr&gt;
Eagle Version 6, Library Revision 2015c, 2015-06-02&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="694108106102">
<description>&lt;b&gt;694108106102&lt;/b&gt;&lt;p&gt;

WR-DC_DC Power Jack_Right Angled_SMT Center Pin Ø2.5_Plug ID Ø2.55_Plug OD Ø5.5_with 4 Soldering Pad &amp; Peg</description>
</package>
</packages>
</library>
<library name="cdclvc-clockbuf">
<packages>
<package name="MSOP12">
<description>12MSOP package according to LTC6957-3 data sheet (LTC DWG# 05-08-1668 Rvv A)</description>
</package>
</packages>
</library>
<library name="ldo">
<description>&lt;b&gt;PCB Matrix Packages&lt;/b&gt;&lt;p&gt;</description>
<packages>
<package name="SOT23L">
</package>
</packages>
</library>
<library name="LED-PLCC2">
<packages>
<package name="PLCC2-MIN">
</package>
</packages>
</library>
<library name="Mentor_lightpipe">
<packages>
<package name="1270.1001">
<description>MENTOR 1270.1001, PCB Mounted 2-Way Right Angle LED Light Pipe, Bi-Level Clear Round Lens</description>
</package>
</packages>
</library>
<library name="oshw">
<description>&lt;p&gt;&lt;strong&gt;Open Source Hardware PCB Logos&lt;/strong&gt;
&lt;p&gt;A simple polygon based version of the OSHWA logos for use on Eagle PCB's
&lt;p&gt;For use please refer to the OSHWA definition at &lt;a href="http://www.oshwa.org/definition/"&gt;http://www.oshwa.org/definition/&lt;/a&gt;
&lt;p&gt;Based on the NBitWonder version (&lt;a href="http://nbitwonder.com"&gt;http://nbitwonder.com&lt;/a&gt;)
&lt;p&gt;&lt;strong&gt;Andrew Cooper&lt;/strong&gt;&lt;br&gt;28Nov2016&lt;br&gt;&lt;a href="http://www.darkerview.com"&gt;www.DarkerView.com&lt;/a&gt;</description>
<packages>
<package name="OSHW_8MM">
</package>
</packages>
</library>
</libraries>
<attributes>
<attribute name="REVISION" value="v1"/>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="rc-sysmocom" package="_0603" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="CAP CER 0.1UF 16V X7R 0603"/>
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics"/>
<attribute name="MANUFACTURERPARTNUMBER" value="CL10B104KO8NNNC"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="1276-1005-1-ND"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/samsung-electro-mechanics/CL10B104KO8NNNC/1276-1005-1-ND/3889091"/>
</element>
<element name="C10" library="rc-sysmocom" package="_0805" value="4.7u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="CAP CER 4.7UF 16V X5R 0805"/>
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics"/>
<attribute name="MANUFACTURERPARTNUMBER" value="CL21A475KOFNNNE"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="1276-1065-1-ND"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/samsung-electro-mechanics/CL21A475KOFNNNE/1276-1065-1-ND/3889151"/>
</element>
<element name="C11" library="rc-sysmocom" package="_0603" value="10n">
<attribute name="DESCRIPTION" value="CAP CER 10000PF 50V X7R 0603"/>
<attribute name="MANUFACTURER" value="KEMET"/>
<attribute name="MANUFACTURERPARTNUMBER" value="C0603C103M5RACTU"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="399-7842-1-ND"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/kemet/C0603C103M5RACTU/399-7842-1-ND/3471565"/>
</element>
<element name="C2" library="rc-sysmocom" package="_0603" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="CAP CER 0.1UF 16V X7R 0603"/>
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics"/>
<attribute name="MANUFACTURERPARTNUMBER" value="CL10B104KO8NNNC"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="1276-1005-1-ND"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/samsung-electro-mechanics/CL10B104KO8NNNC/1276-1005-1-ND/3889091"/>
</element>
<element name="C3" library="rc-sysmocom" package="_0603" value="10n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="CAP CER 10000PF 50V X7R 0603"/>
<attribute name="MANUFACTURER" value="KEMET"/>
<attribute name="MANUFACTURERPARTNUMBER" value="C0603C103M5RACTU"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="399-7842-1-ND"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/kemet/C0603C103M5RACTU/399-7842-1-ND/3471565"/>
</element>
<element name="C4" library="rc-sysmocom" package="_0603" value="10n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="CAP CER 10000PF 50V X7R 0603"/>
<attribute name="MANUFACTURER" value="KEMET"/>
<attribute name="MANUFACTURERPARTNUMBER" value="C0603C103M5RACTU"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="399-7842-1-ND"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/kemet/C0603C103M5RACTU/399-7842-1-ND/3471565"/>
</element>
<element name="C5" library="rc-sysmocom" package="_0603" value="10n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="CAP CER 10000PF 50V X7R 0603"/>
<attribute name="MANUFACTURER" value="KEMET"/>
<attribute name="MANUFACTURERPARTNUMBER" value="C0603C103M5RACTU"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="399-7842-1-ND"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/kemet/C0603C103M5RACTU/399-7842-1-ND/3471565"/>
</element>
<element name="C6" library="rc-sysmocom" package="_0603" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="CAP CER 0.1UF 16V X7R 0603"/>
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics"/>
<attribute name="MANUFACTURERPARTNUMBER" value="CL10B104KO8NNNC"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="1276-1005-1-ND"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/samsung-electro-mechanics/CL10B104KO8NNNC/1276-1005-1-ND/3889091"/>
</element>
<element name="C7" library="rc-sysmocom" package="_0603" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="CAP CER 0.1UF 16V X7R 0603"/>
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics"/>
<attribute name="MANUFACTURERPARTNUMBER" value="CL10B104KO8NNNC"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="1276-1005-1-ND"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/samsung-electro-mechanics/CL10B104KO8NNNC/1276-1005-1-ND/3889091"/>
</element>
<element name="C8" library="rc-sysmocom" package="_0805" value="4.7u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="CAP CER 4.7UF 16V X5R 0805"/>
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics"/>
<attribute name="MANUFACTURERPARTNUMBER" value="CL21A475KOFNNNE"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="1276-1065-1-ND"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/samsung-electro-mechanics/CL21A475KOFNNNE/1276-1065-1-ND/3889151"/>
</element>
<element name="D1" library="laforge" package="0603" value="0603ESDA-TR">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="SUPPRESSOR ESD 30VDC 0603 SMD"/>
<attribute name="MANUFACTURER" value="Eaton - Electronics Division"/>
<attribute name="MANUFACTURERPARTNUMBER" value="0603ESDA2-TR2"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="283-4156-1-ND"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="DIODE"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/eaton-electronics-division/0603ESDA2-TR2/283-4156-1-ND/3681415"/>
</element>
<element name="D2" library="laforge" package="0603" value="0603ESDA-TR">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="SUPPRESSOR ESD 30VDC 0603 SMD"/>
<attribute name="MANUFACTURER" value="Eaton - Electronics Division"/>
<attribute name="MANUFACTURERPARTNUMBER" value="0603ESDA2-TR2"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="283-4156-1-ND"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="DIODE"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/eaton-electronics-division/0603ESDA2-TR2/283-4156-1-ND/3681415"/>
</element>
<element name="D3" library="laforge" package="0603" value="0603ESDA-TR">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="SUPPRESSOR ESD 30VDC 0603 SMD"/>
<attribute name="MANUFACTURER" value="Eaton - Electronics Division"/>
<attribute name="MANUFACTURERPARTNUMBER" value="0603ESDA2-TR2"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="283-4156-1-ND"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="DIODE"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/eaton-electronics-division/0603ESDA2-TR2/283-4156-1-ND/3681415"/>
</element>
<element name="D4" library="laforge" package="0603" value="0603ESDA-TR">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="SUPPRESSOR ESD 30VDC 0603 SMD"/>
<attribute name="MANUFACTURER" value="Eaton - Electronics Division"/>
<attribute name="MANUFACTURERPARTNUMBER" value="0603ESDA2-TR2"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="283-4156-1-ND"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="DIODE"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/eaton-electronics-division/0603ESDA2-TR2/283-4156-1-ND/3681415"/>
</element>
<element name="D5" library="diodes-sysmocom" package="SMADIODE" value="5.6V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="DIODE ZENER 5.6V 3W DO214AC"/>
<attribute name="MANUFACTURER" value="Micro Commercial Co"/>
<attribute name="MANUFACTURERPARTNUMBER" value="3SMAJ5919B-TP"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="3SMAJ5919B-TPMSCT-ND"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="DIODE"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/micro-commercial-co/3SMAJ5919B-TP/3SMAJ5919B-TPMSCT-ND/1793296"/>
</element>
<element name="D6" library="diodes-sysmocom" package="SMADIODE" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="DIODE SCHOTTKY 30V 800MA USC"/>
<attribute name="MANUFACTURER" value="Toshiba Semiconductor and Storage"/>
<attribute name="MANUFACTURERPARTNUMBER" value="CUS08F30,H3F"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="CUS08F30H3FCT-ND"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="DIODE"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/toshiba-semiconductor-and-storage/CUS08F30H3F/CUS08F30H3FCT-ND/5114376"/>
</element>
<element name="F1" library="littlefuse" package="1206L" value="100mA">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="PTC RESET FUSE 30V 200MA 1206"/>
<attribute name="MANUFACTURER" value="Bel Fuse Inc."/>
<attribute name="MANUFACTURERPARTNUMBER" value="0ZCJ0020FF2E"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="507-1797-1-ND"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="UNKNOWN CLASS"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/0ZCJ0020FF2E/507-1797-1-ND/4156228/?itemSeq=282618602"/>
</element>
<element name="JP1" library="jumper" package="JP2" value="FILTA">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="CONN HEADER VERT 3POS 2.54MM"/>
<attribute name="MANUFACTURER" value="Wurth Electronics Inc."/>
<attribute name="MANUFACTURERPARTNUMBER" value="61300311121"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="732-5316-ND"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="CONNECTOR\JUMPER"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/wurth-electronics-inc/61300311121/732-5316-ND/4846825"/>
</element>
<element name="JP2" library="jumper" package="JP2" value="FILTB">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="CONN HEADER VERT 3POS 2.54MM"/>
<attribute name="MANUFACTURER" value="Wurth Electronics Inc."/>
<attribute name="MANUFACTURERPARTNUMBER" value="61300311121"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="732-5316-ND"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="CONNECTOR\JUMPER"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/wurth-electronics-inc/61300311121/732-5316-ND/4846825"/>
</element>
<element name="JP3" library="jumper" package="JP2" value="SD1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="CONN HEADER VERT 3POS 2.54MM"/>
<attribute name="MANUFACTURER" value="Wurth Electronics Inc."/>
<attribute name="MANUFACTURERPARTNUMBER" value="61300311121"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="732-5316-ND"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="CONNECTOR\JUMPER"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/wurth-electronics-inc/61300311121/732-5316-ND/4846825"/>
</element>
<element name="JP4" library="jumper" package="JP2" value="SD2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="CONN HEADER VERT 3POS 2.54MM"/>
<attribute name="MANUFACTURER" value="Wurth Electronics Inc."/>
<attribute name="MANUFACTURERPARTNUMBER" value="61300311121"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="732-5316-ND"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="CONNECTOR\JUMPER"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/wurth-electronics-inc/61300311121/732-5316-ND/4846825"/>
</element>
<element name="JP5" library="laforge" package="1X02" value="DC IN">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="CONN HEADER VERT 2POS 2.54MM"/>
<attribute name="MANUFACTURER" value="Sullins Connector Solutions"/>
<attribute name="MANUFACTURERPARTNUMBER" value="PREC002SAAN-RC"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="S1012EC-02-ND"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="CONNECTOR\JUMPER"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/PREC002SAAN-RC/S1012EC-02-ND/2774852"/>
</element>
<element name="JP6" library="pinhead" package="1X04" value="VDD_SEL">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="CONN HEADER VERT 4POS 2.54MM"/>
<attribute name="MANUFACTURER" value="Sullins Connector Solutions"/>
<attribute name="MANUFACTURERPARTNUMBER" value="PRPC004SAAN-RC"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="S1011EC-04-ND"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="CONNECTOR\JUMPER"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/sullins-connector-solutions/PRPC004SAAN-RC/S1011EC-04-ND/2775250"/>
</element>
<element name="K1" library="Wurth_Elektronik_Electromechanic_DC_Power_Jack_Connectors_rev15c" package="694108106102" value="DC IN">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="CONN PWR JACK 2.5X5.5MM SOLDER"/>
<attribute name="MANUFACTURER" value="Wurth Electronics Inc."/>
<attribute name="MANUFACTURERPARTNUMBER" value="694108106102"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="732-5933-1-ND"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="RELAY"/>
<attribute name="LINK" value="http://www.digikey.de/product-detail/de/wurth-electronics-inc/694108106102/732-5933-1-ND/5047628"/>
</element>
<element name="R1" library="rc-sysmocom" package="_0603" value="330k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="RES 330K OHM 5%% 1/10W 0603"/>
<attribute name="MANUFACTURER" value="Stackpole Electronics Inc"/>
<attribute name="MANUFACTURERPARTNUMBER" value="RMCF0603JG330K"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="RMCF0603JG330KCT-ND"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="RESISTOR"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/stackpole-electronics-inc/RMCF0603JG330K/RMCF0603JG330KCT-ND/6053832"/>
</element>
<element name="R10" library="rc-sysmocom" package="_0603" value="49.9">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="RES 49.9 OHM 1%% 1/10W 0603"/>
<attribute name="MANUFACTURER" value="Stackpole Electronics Inc"/>
<attribute name="MANUFACTURERPARTNUMBER" value="RMCF0603FT49R9"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="RMCF0603FT49R9CT-ND"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="RESISTOR"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/stackpole-electronics-inc/RMCF0603FT49R9/RMCF0603FT49R9CT-ND/1942956"/>
</element>
<element name="R2" library="rc-sysmocom" package="_0603" value="330k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="RES 330K OHM 5%% 1/10W 0603"/>
<attribute name="MANUFACTURER" value="Stackpole Electronics Inc"/>
<attribute name="MANUFACTURERPARTNUMBER" value="RMCF0603JG330K"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="RMCF0603JG330KCT-ND"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="RESISTOR"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/stackpole-electronics-inc/RMCF0603JG330K/RMCF0603JG330KCT-ND/6053832"/>
</element>
<element name="R3" library="rc-sysmocom" package="_0603" value="330k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="RES 330K OHM 5%% 1/10W 0603"/>
<attribute name="MANUFACTURER" value="Stackpole Electronics Inc"/>
<attribute name="MANUFACTURERPARTNUMBER" value="RMCF0603JG330K"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="RMCF0603JG330KCT-ND"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="RESISTOR"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/stackpole-electronics-inc/RMCF0603JG330K/RMCF0603JG330KCT-ND/6053832"/>
</element>
<element name="R4" library="rc-sysmocom" package="_0603" value="330k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="RES 330K OHM 5%% 1/10W 0603"/>
<attribute name="MANUFACTURER" value="Stackpole Electronics Inc"/>
<attribute name="MANUFACTURERPARTNUMBER" value="RMCF0603JG330K"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="RMCF0603JG330KCT-ND"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="RESISTOR"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/stackpole-electronics-inc/RMCF0603JG330K/RMCF0603JG330KCT-ND/6053832"/>
</element>
<element name="R5" library="rc-sysmocom" package="_0603" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="RES 100 OHM 5%% 1/10W 0603"/>
<attribute name="MANUFACTURER" value="Stackpole Electronics Inc"/>
<attribute name="MANUFACTURERPARTNUMBER" value="RMCF0603JT100R"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="RMCF0603JT100RCT-ND"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="RESISTOR"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/stackpole-electronics-inc/RMCF0603JT100R/RMCF0603JT100RCT-ND/1943156"/>
</element>
<element name="R6" library="rc-sysmocom" package="_0603" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="RES 100 OHM 5%% 1/10W 0603"/>
<attribute name="MANUFACTURER" value="Stackpole Electronics Inc"/>
<attribute name="MANUFACTURERPARTNUMBER" value="RMCF0603JT100R"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="RMCF0603JT100RCT-ND"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="RESISTOR"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/stackpole-electronics-inc/RMCF0603JT100R/RMCF0603JT100RCT-ND/1943156"/>
</element>
<element name="R7" library="rc-sysmocom" package="_0603" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="RES 100 OHM 5%% 1/10W 0603"/>
<attribute name="MANUFACTURER" value="Stackpole Electronics Inc"/>
<attribute name="MANUFACTURERPARTNUMBER" value="RMCF0603JT100R"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="RMCF0603JT100RCT-ND"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="RESISTOR"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/stackpole-electronics-inc/RMCF0603JT100R/RMCF0603JT100RCT-ND/1943156"/>
</element>
<element name="R8" library="rc-sysmocom" package="_0603" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="RES 100 OHM 5%% 1/10W 0603"/>
<attribute name="MANUFACTURER" value="Stackpole Electronics Inc"/>
<attribute name="MANUFACTURERPARTNUMBER" value="RMCF0603JT100R"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="RMCF0603JT100RCT-ND"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="RESISTOR"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/stackpole-electronics-inc/RMCF0603JT100R/RMCF0603JT100RCT-ND/1943156"/>
</element>
<element name="R9" library="rc-sysmocom" package="_0603" value="49.9">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="RES 49.9 OHM 1%% 1/10W 0603"/>
<attribute name="MANUFACTURER" value="Stackpole Electronics Inc"/>
<attribute name="MANUFACTURERPARTNUMBER" value="RMCF0603FT49R9"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="RMCF0603FT49R9CT-ND"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="RESISTOR"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/stackpole-electronics-inc/RMCF0603FT49R9/RMCF0603FT49R9CT-ND/1942956"/>
</element>
<element name="U1" library="cdclvc-clockbuf" package="MSOP12" value="LTC6957-4">
<attribute name="NAME"/>
<attribute name="DESCRIPTION" value="IC CLK BUFFER DVR 1:2 12MSOP"/>
<attribute name="MANUFACTURER" value="Linear Technology/Analog Devices"/>
<attribute name="MANUFACTURERPARTNUMBER" value="LTC6957IMS-3#PBF"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="LTC6957IMS-3#PBF-ND"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="IC"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/linear-technology-analog-devices/LTC6957IMS-3-PBF/LTC6957IMS-3-PBF-ND/3973487"/>
</element>
<element name="U2" library="ldo" package="SOT23L" value="ADP151AUJZ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="IC REG LINEAR 3V 200MA TSOT5"/>
<attribute name="MANUFACTURER" value="Analog Devices Inc."/>
<attribute name="MANUFACTURERPARTNUMBER" value="ADP151AUJZ-3.0-R7"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="ADP151AUJZ-3.0-R7CT-ND"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="IC"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/analog-devices-inc/ADP151AUJZ-3.0-R7/ADP151AUJZ-3.0-R7CT-ND/2334207"/>
</element>
<element name="X1" library="laforge" package="HRS_UFL" value="IN+">
<attribute name="OC_DIGIKEY" value="H9161CT-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="CONN U.FL RCPT STR 50 OHM SMD"/>
<attribute name="MANUFACTURER" value="Hirose Electric Co Ltd"/>
<attribute name="MANUFACTURERPARTNUMBER" value="U.FL-R-SMT(10)"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="H9161CT-ND"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="CONNECTOR"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/hirose-electric-co-ltd/U.FL-R-SMT-10/H9161CT-ND/2135256"/>
</element>
<element name="X2" library="laforge" package="HRS_UFL" value="IN-">
<attribute name="OC_DIGIKEY" value="H9161CT-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="CONN U.FL RCPT STR 50 OHM SMD"/>
<attribute name="MANUFACTURER" value="Hirose Electric Co Ltd"/>
<attribute name="MANUFACTURERPARTNUMBER" value="U.FL-R-SMT(10)"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="H9161CT-ND"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="CONNECTOR"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/hirose-electric-co-ltd/U.FL-R-SMT-10/H9161CT-ND/2135256"/>
</element>
<element name="X3" library="laforge" package="HRS_UFL" value="OUT1">
<attribute name="OC_DIGIKEY" value="H9161CT-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="CONN U.FL RCPT STR 50 OHM SMD"/>
<attribute name="MANUFACTURER" value="Hirose Electric Co Ltd"/>
<attribute name="MANUFACTURERPARTNUMBER" value="U.FL-R-SMT(10)"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="H9161CT-ND"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="CONNECTOR"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/hirose-electric-co-ltd/U.FL-R-SMT-10/H9161CT-ND/2135256"/>
</element>
<element name="X4" library="laforge" package="HRS_UFL" value="OUT2">
<attribute name="OC_DIGIKEY" value="H9161CT-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="CONN U.FL RCPT STR 50 OHM SMD"/>
<attribute name="MANUFACTURER" value="Hirose Electric Co Ltd"/>
<attribute name="MANUFACTURERPARTNUMBER" value="U.FL-R-SMT(10)"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="H9161CT-ND"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="CONNECTOR"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/hirose-electric-co-ltd/U.FL-R-SMT-10/H9161CT-ND/2135256"/>
</element>
<element name="X5" library="laforge" package="SMA-F-S-TH" value="IN+">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="CONN SMA JACK R/A 50 OHM PCB"/>
<attribute name="MANUFACTURER" value="TE Connectivity AMP Connectors"/>
<attribute name="MANUFACTURERPARTNUMBER" value="619540-1"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="A120734-ND"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="CONNECTOR"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/te-connectivity-amp-connectors/619540-1/A120734-ND/5021655"/>
</element>
<element name="X6" library="laforge" package="SMA-F-S-TH" value="IN-">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="CONN SMA JACK R/A 50 OHM PCB"/>
<attribute name="MANUFACTURER" value="TE Connectivity AMP Connectors"/>
<attribute name="MANUFACTURERPARTNUMBER" value="619540-1"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="A120734-ND"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="CONNECTOR"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/te-connectivity-amp-connectors/619540-1/A120734-ND/5021655"/>
</element>
<element name="X7" library="laforge" package="SMA-F-S-TH" value="OUT1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="CONN SMA JACK R/A 50 OHM PCB"/>
<attribute name="MANUFACTURER" value="TE Connectivity AMP Connectors"/>
<attribute name="MANUFACTURERPARTNUMBER" value="619540-1"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="A120734-ND"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="CONNECTOR"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/te-connectivity-amp-connectors/619540-1/A120734-ND/5021655"/>
</element>
<element name="X8" library="laforge" package="SMA-F-S-TH" value="OUT2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="CONN SMA JACK R/A 50 OHM PCB"/>
<attribute name="MANUFACTURER" value="TE Connectivity AMP Connectors"/>
<attribute name="MANUFACTURERPARTNUMBER" value="619540-1"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="A120734-ND"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="CONNECTOR"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/te-connectivity-amp-connectors/619540-1/A120734-ND/5021655"/>
</element>
<element name="LED1" library="LED-PLCC2" package="PLCC2-MIN" value="green">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="LED GREEN CLEAR 2PLCC SMD"/>
<attribute name="MANUFACTURER" value="OSRAM Opto Semiconductors Inc."/>
<attribute name="MANUFACTURERPARTNUMBER" value="LG T67F-R1T1-24"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="475-3413-1-ND"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="LED"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/osram-opto-semiconductors-inc/LG-T67F-R1T1-24/475-3413-1-ND/7908021"/>
</element>
<element name="LED2" library="LED-PLCC2" package="PLCC2-MIN" value="yellow">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="LED YELLOW CLEAR 2PLCC SMD"/>
<attribute name="MANUFACTURER" value="OSRAM Opto Semiconductors Inc."/>
<attribute name="MANUFACTURERPARTNUMBER" value="LY T676-S1T1-26-Z"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="475-2665-1-ND"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="LED"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/osram-opto-semiconductors-inc/LY-T676-S1T1-26-Z/475-2665-1-ND"/>
</element>
<element name="M1" library="Mentor_lightpipe" package="1270.1001" value="MENTOR_12701001">
<attribute name="DESCRIPTION" value="NO DESCRIPTION"/>
<attribute name="MANUFACTURER" value="UNKNOWN MANUFACTURER"/>
<attribute name="MANUFACTURERPARTNUMBER" value="UNKNOWN MANUFACTURER PART NUMBER"/>
<attribute name="SOURCE" value="UNKNOWN SOURCE"/>
<attribute name="SOURCEPARTNUMBER" value="UNKNOWN SOURCE PART NUMBER"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="UNKNOWN CLASS"/>
<attribute name="LINK" value="UNKNOWN LINK"/>
</element>
<element name="R11" library="rc-sysmocom" package="_0603" value="330">
<attribute name="DESCRIPTION" value="RES 330 OHM 5%% 1/10W 0603"/>
<attribute name="MANUFACTURER" value="Stackpole Electronics Inc"/>
<attribute name="MANUFACTURERPARTNUMBER" value="RMCF0603JT330R"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="RMCF0603JT330RCT-ND"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="RESISTOR"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/stackpole-electronics-inc/RMCF0603JT330R/RMCF0603JT330RCT-ND/1943164"/>
</element>
<element name="R12" library="rc-sysmocom" package="_0603" value="330">
<attribute name="DESCRIPTION" value="RES 330 OHM 5%% 1/10W 0603"/>
<attribute name="MANUFACTURER" value="Stackpole Electronics Inc"/>
<attribute name="MANUFACTURERPARTNUMBER" value="RMCF0603JT330R"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="RMCF0603JT330RCT-ND"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="RESISTOR"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/stackpole-electronics-inc/RMCF0603JT330R/RMCF0603JT330RCT-ND/1943164"/>
</element>
<element name="C9" library="rc-sysmocom" package="_0603" value="10n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="CAP CER 10000PF 50V X7R 0603"/>
<attribute name="MANUFACTURER" value="KEMET"/>
<attribute name="MANUFACTURERPARTNUMBER" value="C0603C103M5RACTU"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="399-7842-1-ND"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/kemet/C0603C103M5RACTU/399-7842-1-ND/3471565"/>
</element>
<element name="JP7" library="jumper" package="JP1" value="SE">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="CONN HEADER VERT 2POS 2.54MM"/>
<attribute name="MANUFACTURER" value="Sullins Connector Solutions"/>
<attribute name="MANUFACTURERPARTNUMBER" value="PREC002SAAN-RC"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="S1012EC-02-ND"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="CONNECTOR\JUMPER"/>
<attribute name="LINK" value="https://www.digikey.de/product-detail/de/PREC002SAAN-RC/S1012EC-02-ND/2774852"/>
</element>
<element name="U$1" library="oshw" package="OSHW_8MM" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="U1" pad="5"/>
<contactref element="U1" pad="8"/>
<contactref element="U2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="JP1" pad="1"/>
<contactref element="JP2" pad="1"/>
<contactref element="JP3" pad="1"/>
<contactref element="JP4" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="R8" pad="2"/>
<contactref element="R9" pad="2"/>
<contactref element="C8" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="R10" pad="2"/>
<contactref element="X1" pad="GND@1"/>
<contactref element="X1" pad="GND@2"/>
<contactref element="X5" pad="G3"/>
<contactref element="X5" pad="G4"/>
<contactref element="X5" pad="G2"/>
<contactref element="X5" pad="G1"/>
<contactref element="X2" pad="GND@1"/>
<contactref element="X2" pad="GND@2"/>
<contactref element="X6" pad="G1"/>
<contactref element="X6" pad="G2"/>
<contactref element="X6" pad="G3"/>
<contactref element="X6" pad="G4"/>
<contactref element="D2" pad="1"/>
<contactref element="D3" pad="1"/>
<contactref element="X3" pad="GND@2"/>
<contactref element="X3" pad="GND@1"/>
<contactref element="X7" pad="G4"/>
<contactref element="X7" pad="G3"/>
<contactref element="X7" pad="G2"/>
<contactref element="X7" pad="G1"/>
<contactref element="X4" pad="GND@2"/>
<contactref element="X4" pad="GND@1"/>
<contactref element="X8" pad="G1"/>
<contactref element="X8" pad="G2"/>
<contactref element="X8" pad="G3"/>
<contactref element="X8" pad="G4"/>
<contactref element="D4" pad="1"/>
<contactref element="D1" pad="1"/>
<contactref element="D5" pad="A"/>
<contactref element="JP5" pad="2"/>
<contactref element="K1" pad="3"/>
<contactref element="K1" pad="2"/>
<contactref element="JP6" pad="4"/>
<contactref element="LED1" pad="K"/>
<contactref element="LED2" pad="K"/>
<contactref element="C9" pad="2"/>
</signal>
<signal name="VDD">
<contactref element="U1" pad="11"/>
<contactref element="C2" pad="1"/>
<contactref element="JP6" pad="3"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="FILTA">
<contactref element="U1" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="FILTB">
<contactref element="U1" pad="6"/>
<contactref element="R2" pad="1"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="SD1">
<contactref element="U1" pad="12"/>
<contactref element="R3" pad="1"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="SD2">
<contactref element="U1" pad="7"/>
<contactref element="R4" pad="1"/>
<contactref element="JP4" pad="2"/>
</signal>
<signal name="V+">
<contactref element="JP1" pad="3"/>
<contactref element="JP4" pad="3"/>
<contactref element="JP3" pad="3"/>
<contactref element="JP2" pad="3"/>
<contactref element="U1" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="U2" pad="5"/>
<contactref element="C7" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="JP6" pad="2"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="10"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="C3" pad="1"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="OUT1">
<contactref element="R5" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="X3" pad="SIG"/>
<contactref element="D3" pad="2"/>
<contactref element="X7" pad="C"/>
</signal>
<signal name="N$8">
<contactref element="U1" pad="9"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="C4" pad="1"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="OUT2">
<contactref element="R7" pad="1"/>
<contactref element="R8" pad="1"/>
<contactref element="X4" pad="SIG"/>
<contactref element="D4" pad="2"/>
<contactref element="X8" pad="C"/>
</signal>
<signal name="IN+">
<contactref element="U1" pad="3"/>
<contactref element="C5" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="C5" pad="2"/>
<contactref element="R9" pad="1"/>
<contactref element="X1" pad="SIG"/>
<contactref element="D1" pad="2"/>
<contactref element="X5" pad="C"/>
</signal>
<signal name="V_IN">
<contactref element="C8" pad="2"/>
<contactref element="U2" pad="1"/>
<contactref element="U2" pad="3"/>
<contactref element="C6" pad="2"/>
<contactref element="F1" pad="1"/>
<contactref element="D5" pad="C"/>
<contactref element="JP6" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="U1" pad="4"/>
<contactref element="C11" pad="1"/>
<contactref element="JP7" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="C11" pad="2"/>
<contactref element="R10" pad="1"/>
<contactref element="X2" pad="SIG"/>
<contactref element="D2" pad="2"/>
<contactref element="X6" pad="C"/>
</signal>
<signal name="N$5">
<contactref element="D6" pad="C"/>
<contactref element="F1" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="JP5" pad="1"/>
<contactref element="D6" pad="A"/>
<contactref element="K1" pad="1"/>
<contactref element="K1" pad="1-1"/>
</signal>
<signal name="N$1">
<contactref element="LED1" pad="A"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="LED2" pad="A"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="C9" pad="1"/>
<contactref element="JP7" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
