<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="-20" y1="0" x2="50" y2="0" width="0" layer="20"/>
<wire x1="50" y1="0" x2="50" y2="70" width="0" layer="20"/>
<wire x1="50" y1="70" x2="-20" y2="70" width="0" layer="20"/>
<wire x1="-20" y1="70" x2="-20" y2="0" width="0" layer="20"/>
<text>miniPCIe breakout</text>
<text>(C) 2016 Harald Welte
Mfg: sysmocom GmbH
License: CC-BY-SA</text>
<text>&gt;VERSION</text>
<text>miniPCIe breakout</text>
<text>(C) 2016 Harald Welte
Mfg: sysmocom GmbH
License: CC-BY-SA</text>
<text>&gt;VERSION</text>
<text>1</text>
<text>USB</text>
<text>DC IN</text>
<text>PERST</text>
<text>W_DIS</text>
<text>5V DC</text>
</plain>
<libraries>
<library name="con-miniPCIe">
<description>
</description>
<packages>
<package name="MM60-52">
<description>JAE MM60-52</description>
</package>
</packages>
</library>
<library name="con-hirose">
<description>&lt;b&gt;Hirose Connectors&lt;/b&gt;&lt;p&gt;
www.hirose.co.jp&lt;p&gt;
Include : &lt;br&gt;
con-hirose-df12d(3.0)60dp0.5v80.lbr from Bob Starr &amp;lt;rtzaudio@mindspring.com&amp;gt;&lt;br&gt;
con-hirose.lbr from Bob Starr &amp;lt;rtzaudio@mindspring.com&amp;gt;&lt;br&gt;</description>
<packages>
<package name="UX60-MB-5ST">
<description>&lt;b&gt;MINI USB Connector HI-SPEED Certified&lt;/b&gt; Metal Shield SMT Type With Positioning Post&lt;p&gt;
Source: http://www.hirose.co.jp/cataloge_hp/e24000019.pdf</description>
</package>
</packages>
</library>
<library name="SF7W008S1A-SIM">
<packages>
<package name="SF7W008S1A-RESTR">
<description>JAE SF7W008S1A SIM card holder with lock and card detect switch - additional restrict areas for SIM contacts</description>
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="CHIP-LED0603">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB Q993&lt;br&gt;
Source: http://www.osram.convergy.de/ ... Lb_q993.pdf</description>
</package>
</packages>
</library>
<library name="jumper">
<description>&lt;b&gt;Jumpers&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="JP1">
<description>&lt;b&gt;JUMPER&lt;/b&gt;</description>
</package>
<package name="JP2">
<description>&lt;b&gt;JUMPER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="rc-sysmocom">
<packages>
<package name="_0603">
<description>&lt;b&gt;0603&lt;/b&gt;</description>
</package>
<package name="_0805">
<description>&lt;b&gt;0805&lt;/b&gt;</description>
</package>
<package name="_0402">
<description>&lt;b&gt; 0402&lt;/b&gt;</description>
</package>
<package name="1206">
<description>&lt;b&gt;1206 (3216 Metric)&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="laforge">
<description>&lt;b&gt;PCB Matrix Packages&lt;/b&gt;&lt;p&gt;</description>
<packages>
<package name="TSOP-6">
<description>TSOP-6 CAS E318G-02 ISSUE V (ON Semiconductor)</description>
</package>
<package name="SMA-F-S-TH">
</package>
<package name="HRS_UFL">
<description>&lt;b&gt;Hirose U.FL SMT&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="ldo">
<description>&lt;b&gt;PCB Matrix Packages&lt;/b&gt;&lt;p&gt;</description>
<packages>
<package name="ST_D2PAK">
<description>D2PAK footprint according to DocID6378 Rev 27 / LD0185 data sheet</description>
</package>
</packages>
</library>
<library name="Wurth_Elektronik_Electromechanic_DC_Power_Jack_Connectors_rev15c">
<description>&lt;BR&gt;Wurth Elektronik - DC Power Jack Connectors&lt;br&gt;&lt;Hr&gt;
&lt;BR&gt;&lt;BR&gt; 
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-405&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/eagle"&gt;http://www.we-online.com/eagle &lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither CadSoft nor WE-eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;&lt;BR&gt;&lt;br&gt;
&lt;hr&gt;
Eagle Version 6, Library Revision 2015c, 2015-06-02&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="694108106102">
<description>&lt;b&gt;694108106102&lt;/b&gt;&lt;p&gt;

WR-DC_DC Power Jack_Right Angled_SMT Center Pin Ø2.5_Plug ID Ø2.55_Plug OD Ø5.5_with 4 Soldering Pad &amp; Peg</description>
</package>
</packages>
</library>
<library name="rcl">
<description>&lt;b&gt;Resistors, Capacitors, Inductors&lt;/b&gt;&lt;p&gt;
Based on the previous libraries:
&lt;ul&gt;
&lt;li&gt;r.lbr
&lt;li&gt;cap.lbr 
&lt;li&gt;cap-fe.lbr
&lt;li&gt;captant.lbr
&lt;li&gt;polcap.lbr
&lt;li&gt;ipc-smd.lbr
&lt;/ul&gt;
All SMD packages are defined according to the IPC specifications and  CECC&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;p&gt;
&lt;p&gt;
for Electrolyt Capacitors see also :&lt;p&gt;
www.bccomponents.com &lt;p&gt;
www.panasonic.com&lt;p&gt;
www.kemet.com&lt;p&gt;
http://www.secc.co.jp/pdf/os_e/2004/e_os_all.pdf &lt;b&gt;(SANYO)&lt;/b&gt;
&lt;p&gt;
for trimmer refence see : &lt;u&gt;www.electrospec-inc.com/cross_references/trimpotcrossref.asp&lt;/u&gt;&lt;p&gt;

&lt;table border=0 cellspacing=0 cellpadding=0 width="100%" cellpaddding=0&gt;
&lt;tr valign="top"&gt;

&lt;! &lt;td width="10"&gt;&amp;nbsp;&lt;/td&gt;
&lt;td width="90%"&gt;

&lt;b&gt;&lt;font color="#0000FF" size="4"&gt;TRIM-POT CROSS REFERENCE&lt;/font&gt;&lt;/b&gt;
&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;RECTANGULAR MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BOURNS&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BI&amp;nbsp;TECH&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;DALE-VISHAY&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PHILIPS/MEPCO&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MURATA&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PANASONIC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;SPECTROL&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MILSPEC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;&lt;TD&gt;&amp;nbsp;&lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3 &gt;
      3005P&lt;BR&gt;
      3006P&lt;BR&gt;
      3006W&lt;BR&gt;
      3006Y&lt;BR&gt;
      3009P&lt;BR&gt;
      3009W&lt;BR&gt;
      3009Y&lt;BR&gt;
      3057J&lt;BR&gt;
      3057L&lt;BR&gt;
      3057P&lt;BR&gt;
      3057Y&lt;BR&gt;
      3059J&lt;BR&gt;
      3059L&lt;BR&gt;
      3059P&lt;BR&gt;
      3059Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      89P&lt;BR&gt;
      89W&lt;BR&gt;
      89X&lt;BR&gt;
      89PH&lt;BR&gt;
      76P&lt;BR&gt;
      89XH&lt;BR&gt;
      78SLT&lt;BR&gt;
      78L&amp;nbsp;ALT&lt;BR&gt;
      56P&amp;nbsp;ALT&lt;BR&gt;
      78P&amp;nbsp;ALT&lt;BR&gt;
      T8S&lt;BR&gt;
      78L&lt;BR&gt;
      56P&lt;BR&gt;
      78P&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      T18/784&lt;BR&gt;
      783&lt;BR&gt;
      781&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2199&lt;BR&gt;
      1697/1897&lt;BR&gt;
      1680/1880&lt;BR&gt;
      2187&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      8035EKP/CT20/RJ-20P&lt;BR&gt;
      -&lt;BR&gt;
      RJ-20X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      1211L&lt;BR&gt;
      8012EKQ&amp;nbsp;ALT&lt;BR&gt;
      8012EKR&amp;nbsp;ALT&lt;BR&gt;
      1211P&lt;BR&gt;
      8012EKJ&lt;BR&gt;
      8012EKL&lt;BR&gt;
      8012EKQ&lt;BR&gt;
      8012EKR&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      2101P&lt;BR&gt;
      2101W&lt;BR&gt;
      2101Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2102L&lt;BR&gt;
      2102S&lt;BR&gt;
      2102Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVMCOG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      43P&lt;BR&gt;
      43W&lt;BR&gt;
      43Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      40L&lt;BR&gt;
      40P&lt;BR&gt;
      40Y&lt;BR&gt;
      70Y-T602&lt;BR&gt;
      70L&lt;BR&gt;
      70P&lt;BR&gt;
      70Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SQUARE MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
   &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3250L&lt;BR&gt;
      3250P&lt;BR&gt;
      3250W&lt;BR&gt;
      3250X&lt;BR&gt;
      3252P&lt;BR&gt;
      3252W&lt;BR&gt;
      3252X&lt;BR&gt;
      3260P&lt;BR&gt;
      3260W&lt;BR&gt;
      3260X&lt;BR&gt;
      3262P&lt;BR&gt;
      3262W&lt;BR&gt;
      3262X&lt;BR&gt;
      3266P&lt;BR&gt;
      3266W&lt;BR&gt;
      3266X&lt;BR&gt;
      3290H&lt;BR&gt;
      3290P&lt;BR&gt;
      3290W&lt;BR&gt;
      3292P&lt;BR&gt;
      3292W&lt;BR&gt;
      3292X&lt;BR&gt;
      3296P&lt;BR&gt;
      3296W&lt;BR&gt;
      3296X&lt;BR&gt;
      3296Y&lt;BR&gt;
      3296Z&lt;BR&gt;
      3299P&lt;BR&gt;
      3299W&lt;BR&gt;
      3299X&lt;BR&gt;
      3299Y&lt;BR&gt;
      3299Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64P&amp;nbsp;ALT&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      64X&amp;nbsp;ALT&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66P&lt;BR&gt;
      66W&lt;BR&gt;
      66X&lt;BR&gt;
      67P&lt;BR&gt;
      67W&lt;BR&gt;
      67X&lt;BR&gt;
      67Y&lt;BR&gt;
      67Z&lt;BR&gt;
      68P&lt;BR&gt;
      68W&lt;BR&gt;
      68X&lt;BR&gt;
      67Y&amp;nbsp;ALT&lt;BR&gt;
      67Z&amp;nbsp;ALT&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      5050&lt;BR&gt;
      5091&lt;BR&gt;
      5080&lt;BR&gt;
      5087&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T63YB&lt;BR&gt;
      T63XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      5887&lt;BR&gt;
      5891&lt;BR&gt;
      5880&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T93Z&lt;BR&gt;
      T93YA&lt;BR&gt;
      T93XA&lt;BR&gt;
      T93YB&lt;BR&gt;
      T93XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKW&lt;BR&gt;
      8026EKM&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKB&lt;BR&gt;
      8026EKM&lt;BR&gt;
      1309X&lt;BR&gt;
      1309P&lt;BR&gt;
      1309W&lt;BR&gt;
      8024EKP&lt;BR&gt;
      8024EKW&lt;BR&gt;
      8024EKN&lt;BR&gt;
      RJ-9P/CT9P&lt;BR&gt;
      RJ-9W&lt;BR&gt;
      RJ-9X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3105P/3106P&lt;BR&gt;
      3105W/3106W&lt;BR&gt;
      3105X/3106X&lt;BR&gt;
      3105Y/3106Y&lt;BR&gt;
      3105Z/3105Z&lt;BR&gt;
      3102P&lt;BR&gt;
      3102W&lt;BR&gt;
      3102X&lt;BR&gt;
      3102Y&lt;BR&gt;
      3102Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMCBG&lt;BR&gt;
      EVMCCG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      55-1-X&lt;BR&gt;
      55-4-X&lt;BR&gt;
      55-3-X&lt;BR&gt;
      55-2-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      50-2-X&lt;BR&gt;
      50-4-X&lt;BR&gt;
      50-3-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      64Y&lt;BR&gt;
      64Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3323P&lt;BR&gt;
      3323S&lt;BR&gt;
      3323W&lt;BR&gt;
      3329H&lt;BR&gt;
      3329P&lt;BR&gt;
      3329W&lt;BR&gt;
      3339H&lt;BR&gt;
      3339P&lt;BR&gt;
      3339W&lt;BR&gt;
      3352E&lt;BR&gt;
      3352H&lt;BR&gt;
      3352K&lt;BR&gt;
      3352P&lt;BR&gt;
      3352T&lt;BR&gt;
      3352V&lt;BR&gt;
      3352W&lt;BR&gt;
      3362H&lt;BR&gt;
      3362M&lt;BR&gt;
      3362P&lt;BR&gt;
      3362R&lt;BR&gt;
      3362S&lt;BR&gt;
      3362U&lt;BR&gt;
      3362W&lt;BR&gt;
      3362X&lt;BR&gt;
      3386B&lt;BR&gt;
      3386C&lt;BR&gt;
      3386F&lt;BR&gt;
      3386H&lt;BR&gt;
      3386K&lt;BR&gt;
      3386M&lt;BR&gt;
      3386P&lt;BR&gt;
      3386S&lt;BR&gt;
      3386W&lt;BR&gt;
      3386X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      25P&lt;BR&gt;
      25S&lt;BR&gt;
      25RX&lt;BR&gt;
      82P&lt;BR&gt;
      82M&lt;BR&gt;
      82PA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      91E&lt;BR&gt;
      91X&lt;BR&gt;
      91T&lt;BR&gt;
      91B&lt;BR&gt;
      91A&lt;BR&gt;
      91V&lt;BR&gt;
      91W&lt;BR&gt;
      25W&lt;BR&gt;
      25V&lt;BR&gt;
      25P&lt;BR&gt;
      -&lt;BR&gt;
      25S&lt;BR&gt;
      25U&lt;BR&gt;
      25RX&lt;BR&gt;
      25X&lt;BR&gt;
      72XW&lt;BR&gt;
      72XL&lt;BR&gt;
      72PM&lt;BR&gt;
      72RX&lt;BR&gt;
      -&lt;BR&gt;
      72PX&lt;BR&gt;
      72P&lt;BR&gt;
      72RXW&lt;BR&gt;
      72RXL&lt;BR&gt;
      72X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T7YB&lt;BR&gt;
      T7YA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      TXD&lt;BR&gt;
      TYA&lt;BR&gt;
      TYP&lt;BR&gt;
      -&lt;BR&gt;
      TYD&lt;BR&gt;
      TX&lt;BR&gt;
      -&lt;BR&gt;
      150SX&lt;BR&gt;
      100SX&lt;BR&gt;
      102T&lt;BR&gt;
      101S&lt;BR&gt;
      190T&lt;BR&gt;
      150TX&lt;BR&gt;
      101&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      101SX&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ET6P&lt;BR&gt;
      ET6S&lt;BR&gt;
      ET6X&lt;BR&gt;
      RJ-6W/8014EMW&lt;BR&gt;
      RJ-6P/8014EMP&lt;BR&gt;
      RJ-6X/8014EMX&lt;BR&gt;
      TM7W&lt;BR&gt;
      TM7P&lt;BR&gt;
      TM7X&lt;BR&gt;
      -&lt;BR&gt;
      8017SMS&lt;BR&gt;
      -&lt;BR&gt;
      8017SMB&lt;BR&gt;
      8017SMA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      CT-6W&lt;BR&gt;
      CT-6H&lt;BR&gt;
      CT-6P&lt;BR&gt;
      CT-6R&lt;BR&gt;
      -&lt;BR&gt;
      CT-6V&lt;BR&gt;
      CT-6X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKV&lt;BR&gt;
      -&lt;BR&gt;
      8038EKX&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKP&lt;BR&gt;
      8038EKZ&lt;BR&gt;
      8038EKW&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3321H&lt;BR&gt;
      3321P&lt;BR&gt;
      3321N&lt;BR&gt;
      1102H&lt;BR&gt;
      1102P&lt;BR&gt;
      1102T&lt;BR&gt;
      RVA0911V304A&lt;BR&gt;
      -&lt;BR&gt;
      RVA0911H413A&lt;BR&gt;
      RVG0707V100A&lt;BR&gt;
      RVA0607V(H)306A&lt;BR&gt;
      RVA1214H213A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3104B&lt;BR&gt;
      3104C&lt;BR&gt;
      3104F&lt;BR&gt;
      3104H&lt;BR&gt;
      -&lt;BR&gt;
      3104M&lt;BR&gt;
      3104P&lt;BR&gt;
      3104S&lt;BR&gt;
      3104W&lt;BR&gt;
      3104X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      EVMQ0G&lt;BR&gt;
      EVMQIG&lt;BR&gt;
      EVMQ3G&lt;BR&gt;
      EVMS0G&lt;BR&gt;
      EVMQ0G&lt;BR&gt;
      EVMG0G&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMK4GA00B&lt;BR&gt;
      EVM30GA00B&lt;BR&gt;
      EVMK0GA00B&lt;BR&gt;
      EVM38GA00B&lt;BR&gt;
      EVMB6&lt;BR&gt;
      EVLQ0&lt;BR&gt;
      -&lt;BR&gt;
      EVMMSG&lt;BR&gt;
      EVMMBG&lt;BR&gt;
      EVMMAG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMMCS&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM0&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM3&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      62-3-1&lt;BR&gt;
      62-1-2&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67R&lt;BR&gt;
      -&lt;BR&gt;
      67P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67X&lt;BR&gt;
      63V&lt;BR&gt;
      63S&lt;BR&gt;
      63M&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63H&lt;BR&gt;
      63P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;&amp;nbsp;&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=3&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT color="#0000FF" SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SMD TRIM-POT CROSS REFERENCE&lt;/B&gt;&lt;/FONT&gt;
      &lt;P&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3224G&lt;BR&gt;
      3224J&lt;BR&gt;
      3224W&lt;BR&gt;
      3269P&lt;BR&gt;
      3269W&lt;BR&gt;
      3269X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      44G&lt;BR&gt;
      44J&lt;BR&gt;
      44W&lt;BR&gt;
      84P&lt;BR&gt;
      84W&lt;BR&gt;
      84X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST63Z&lt;BR&gt;
      ST63Y&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST5P&lt;BR&gt;
      ST5W&lt;BR&gt;
      ST5X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3314G&lt;BR&gt;
      3314J&lt;BR&gt;
      3364A/B&lt;BR&gt;
      3364C/D&lt;BR&gt;
      3364W/X&lt;BR&gt;
      3313G&lt;BR&gt;
      3313J&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      23B&lt;BR&gt;
      23A&lt;BR&gt;
      21X&lt;BR&gt;
      21W&lt;BR&gt;
      -&lt;BR&gt;
      22B&lt;BR&gt;
      22A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST5YL/ST53YL&lt;BR&gt;
      ST5YJ/5T53YJ&lt;BR&gt;
      ST-23A&lt;BR&gt;
      ST-22B&lt;BR&gt;
      ST-22&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST-4B&lt;BR&gt;
      ST-4A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST-3B&lt;BR&gt;
      ST-3A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVM-6YS&lt;BR&gt;
      EVM-1E&lt;BR&gt;
      EVM-1G&lt;BR&gt;
      EVM-1D&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      G4B&lt;BR&gt;
      G4A&lt;BR&gt;
      TR04-3S1&lt;BR&gt;
      TRG04-2S1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      DVR-43A&lt;BR&gt;
      CVR-42C&lt;BR&gt;
      CVR-42A/C&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;
&lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;ALT =&amp;nbsp;ALTERNATE&lt;/B&gt;&lt;/FONT&gt;
&lt;P&gt;

&amp;nbsp;
&lt;P&gt;
&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;</description>
<packages>
<package name="UD-8X10_NICHICON">
<description>&lt;b&gt;ALUMINUM ELECTROLYTIC CAPACITORS&lt;/b&gt; UD Series 8 x 10 mm&lt;p&gt;
Source: http://products.nichicon.co.jp/en/pdf/XJA043/e-ud.pdf</description>
</package>
<package name="SMC_E">
<description>&lt;b&gt;Chip Capacitor &lt;/b&gt; Polar tantalum capacitors with solid electrolyte&lt;p&gt;
Siemens Matsushita Components B 45 194, B 45 197, B 45 198&lt;br&gt;
Source: www.farnell.com/datasheets/247.pdf</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2X12">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
<attribute name="VERSION" value="v3"/>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="X1" library="con-miniPCIe" package="MM60-52" value="MPCIE-JAE">
<attribute name="DESCRIPTION" value="CONN MINI EXPRESS CARD 52POS SMD"/>
<attribute name="MANUFACTURER" value="JAE Electronics"/>
<attribute name="MANUFACTURERPARTNUMBER" value="MM60-52B1-E1-R650"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="670-2275-1-ND"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="CONNECTOR"/>
<attribute name="LINK" value="http://www.digikey.com/product-detail/en/jae-electronics/MM60-52B1-E1-R650/670-2275-1-ND"/>
</element>
<element name="X2" library="con-hirose" package="UX60-MB-5ST" value="MINI-USB-SHIELD-UX60-MB-5ST">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="USB - mini B USB 2.0 Receptacle Connector 5 Position Surface Mount, Right Angle, Horizontal"/>
<attribute name="MANUFACTURER" value="Hirose Electric Co Ltd"/>
<attribute name="MANUFACTURERPARTNUMBER" value="UX60-MB-5ST"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="H2959CT-ND"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="CONNECTOR"/>
<attribute name="LINK" value="http://www.digikey.com/product-detail/en/hirose-electric-co-ltd/UX60-MB-5ST/H2959CT-ND/597538"/>
</element>
<element name="SIM1" library="SF7W008S1A-SIM" package="SF7W008S1A-RESTR" value="SF7W008S1A-R">
<attribute name="OC_DIGIKEY" value="670-2337-1-ND"/>
<attribute name="DESCRIPTION" value="8 (6 + 2) Position Card Connector SIM Card Surface Mount, Right Angle Gold"/>
<attribute name="MANUFACTURER" value="JAE Electronics"/>
<attribute name="MANUFACTURERPARTNUMBER" value="SF7W008S1AE900"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="670-2337-1-ND"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="UNKNOWN CLASS"/>
<attribute name="LINK" value="http://www.digikey.com/product-detail/en/jae-electronics/SF7W008S1AE900/670-2337-1-ND/1284033"/>
</element>
<element name="LED1" library="led" package="CHIP-LED0603" value="YELLOW">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="NO DESCRIPTION"/>
<attribute name="MANUFACTURER" value="UNKNOWN MANUFACTURER"/>
<attribute name="MANUFACTURERPARTNUMBER" value="UNKNOWN MANUFACTURER PART NUMBER"/>
<attribute name="SOURCE" value="UNKNOWN SOURCE"/>
<attribute name="SOURCEPARTNUMBER" value="UNKNOWN SOURCE PART NUMBER"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="LED"/>
<attribute name="LINK" value="UNKNOWN LINK"/>
</element>
<element name="JP1" library="jumper" package="JP1" value="">
<attribute name="DESCRIPTION" value="NO DESCRIPTION"/>
<attribute name="MANUFACTURER" value="UNKNOWN MANUFACTURER"/>
<attribute name="MANUFACTURERPARTNUMBER" value="UNKNOWN MANUFACTURER PART NUMBER"/>
<attribute name="SOURCE" value="UNKNOWN SOURCE"/>
<attribute name="SOURCEPARTNUMBER" value="UNKNOWN SOURCE PART NUMBER"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="CONNECTOR\JUMPER"/>
<attribute name="LINK" value="UNKNOWN LINK"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="jumper" package="JP1" value="">
<attribute name="DESCRIPTION" value="NO DESCRIPTION"/>
<attribute name="MANUFACTURER" value="UNKNOWN MANUFACTURER"/>
<attribute name="MANUFACTURERPARTNUMBER" value="UNKNOWN MANUFACTURER PART NUMBER"/>
<attribute name="SOURCE" value="UNKNOWN SOURCE"/>
<attribute name="SOURCEPARTNUMBER" value="UNKNOWN SOURCE PART NUMBER"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="CONNECTOR\JUMPER"/>
<attribute name="LINK" value="UNKNOWN LINK"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="rc-sysmocom" package="_0603" value="47">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="RES SMD 47 OHM 5% 1/10W 0603"/>
<attribute name="MANUFACTURER" value="Yageo"/>
<attribute name="MANUFACTURERPARTNUMBER" value="RC0603JR-0747RL"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="311-47GRCT-ND"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="RESISTOR"/>
<attribute name="LINK" value="http://www.digikey.com/product-detail/en/yageo/RC0603JR-0747RL/311-47GRCT-ND/729740"/>
</element>
<element name="R2" library="rc-sysmocom" package="_0603" value="47">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="RES SMD 47 OHM 5% 1/10W 0603"/>
<attribute name="MANUFACTURER" value="Yageo"/>
<attribute name="MANUFACTURERPARTNUMBER" value="RC0603JR-0747RL"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="311-47GRCT-ND"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="RESISTOR"/>
<attribute name="LINK" value="http://www.digikey.com/product-detail/en/yageo/RC0603JR-0747RL/311-47GRCT-ND/729740"/>
</element>
<element name="R3" library="rc-sysmocom" package="_0603" value="47">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="RES SMD 47 OHM 5% 1/10W 0603"/>
<attribute name="MANUFACTURER" value="Yageo"/>
<attribute name="MANUFACTURERPARTNUMBER" value="RC0603JR-0747RL"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="311-47GRCT-ND"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="RESISTOR"/>
<attribute name="LINK" value="http://www.digikey.com/product-detail/en/yageo/RC0603JR-0747RL/311-47GRCT-ND/729740"/>
</element>
<element name="U1" library="laforge" package="TSOP-6" value="IP4234CZ6">
<attribute name="OC_DIGIKEY" value="568-5869-1-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="TVS DIODE 5.5VWM 6TSOP"/>
<attribute name="MANUFACTURER" value="NXP Semiconductors"/>
<attribute name="MANUFACTURERPARTNUMBER" value="IP4234CZ6,125"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="568-5869-1-ND"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="IC"/>
<attribute name="LINK" value="http://www.digikey.com/product-detail/en/nxp-semiconductors/IP4234CZ6,125/568-5869-1-ND/2531156"/>
</element>
<element name="U2" library="ldo" package="ST_D2PAK" value="LD1085D2T33R">
<attribute name="DESCRIPTION" value="Linear Voltage Regulator IC Positive Fixed 1 Output 3.3V 3A D2PAK"/>
<attribute name="MANUFACTURER" value="STMicroelectronics"/>
<attribute name="MANUFACTURERPARTNUMBER" value="LD1085D2T33R"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="497-1222-1-ND"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="IC"/>
<attribute name="LINK" value="http://www.digikey.com/product-detail/en/stmicroelectronics/LD1085D2T33R/497-1222-1-ND/586222"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="rc-sysmocom" package="_0805" value="10u">
<attribute name="DESCRIPTION" value="10µF 16V Ceramic Capacitor X5R 0805 (2012 Metric) 0.079&quot; L x 0.049&quot; W (2.00mm x 1.25mm)"/>
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics America, Inc."/>
<attribute name="MANUFACTURERPARTNUMBER" value="CL21A106KOQNNNG"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="1276-6455-1-ND"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="LINK" value="http://www.digikey.com/product-detail/en/samsung-electro-mechanics-america-inc/CL21A106KOQNNNG/1276-6455-1-ND/5958083"/>
</element>
<element name="C2" library="rc-sysmocom" package="_0805" value="10u">
<attribute name="DESCRIPTION" value="10µF 16V Ceramic Capacitor X5R 0805 (2012 Metric) 0.079&quot; L x 0.049&quot; W (2.00mm x 1.25mm)"/>
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics America, Inc."/>
<attribute name="MANUFACTURERPARTNUMBER" value="CL21A106KOQNNNG"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="1276-6455-1-ND"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="LINK" value="http://www.digikey.com/product-detail/en/samsung-electro-mechanics-america-inc/CL21A106KOQNNNG/1276-6455-1-ND/5958083"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="K1" library="Wurth_Elektronik_Electromechanic_DC_Power_Jack_Connectors_rev15c" package="694108106102" value="694108106102">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="Power Barrel Connector Jack 2.50mm ID (0.098&quot;), 5.50mm OD (0.217&quot;) Surface Mount, Right Angle"/>
<attribute name="MANUFACTURER" value="Wurth Electronics Inc"/>
<attribute name="MANUFACTURERPARTNUMBER" value="694108106102"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="732-5933-1-ND"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="RELAY"/>
<attribute name="LINK" value="http://www.digikey.com/product-detail/en/wurth-electronics-inc/694108106102/732-5933-1-ND/5047628"/>
</element>
<element name="JP3" library="jumper" package="JP2" value="">
<attribute name="DESCRIPTION" value="NO DESCRIPTION"/>
<attribute name="MANUFACTURER" value="UNKNOWN MANUFACTURER"/>
<attribute name="MANUFACTURERPARTNUMBER" value="UNKNOWN MANUFACTURER PART NUMBER"/>
<attribute name="SOURCE" value="UNKNOWN SOURCE"/>
<attribute name="SOURCEPARTNUMBER" value="UNKNOWN SOURCE PART NUMBER"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="CONNECTOR\JUMPER"/>
<attribute name="LINK" value="UNKNOWN LINK"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="rcl" package="UD-8X10_NICHICON" value="470u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="470µF 6.3V Aluminum Capacitors Radial, Can - SMD  2000 Hrs @ 85°C"/>
<attribute name="MANUFACTURER" value="Nichicon"/>
<attribute name="MANUFACTURERPARTNUMBER" value="UUR0J471MNL1GS"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="493-6207-1-ND"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="LINK" value="http://www.digikey.com/product-detail/en/nichicon/UUR0J471MNL1GS/493-6207-1-ND/3438720"/>
</element>
<element name="C4" library="rcl" package="SMC_E" value="DNP">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="NO DESCRIPTION"/>
<attribute name="MANUFACTURER" value="UNKNOWN MANUFACTURER"/>
<attribute name="MANUFACTURERPARTNUMBER" value="UNKNOWN MANUFACTURER PART NUMBER"/>
<attribute name="SOURCE" value="UNKNOWN SOURCE"/>
<attribute name="SOURCEPARTNUMBER" value="UNKNOWN SOURCE PART NUMBER"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="FALSE"/>
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="LINK" value="UNKNOWN LINK"/>
</element>
<element name="C107" library="rc-sysmocom" package="_0402" value="33p">
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics America, Inc."/>
<attribute name="SOURCEPARTNUMBER" value="1276-1272-1-ND"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="LINK" value="http://www.digikey.com/product-detail/en/CL05C330JB5NNNC/1276-1272-1-ND/3889358"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="MANUFACTURERPARTNUMBER" value="CL05C330JB5NNNC"/>
<attribute name="DESCRIPTION" value="CAP CER 33PF 50V NP0 0402"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C108" library="rc-sysmocom" package="_0603" value="10p">
<attribute name="MANUFACTURER" value="Kemet"/>
<attribute name="SOURCEPARTNUMBER" value="399-1049-1-ND"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="LINK" value="http://www.digikey.com/product-detail/en/C0603C100J5GACTU/399-1049-1-ND"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="MANUFACTURERPARTNUMBER" value="C0603C100J5GACTU"/>
<attribute name="DESCRIPTION" value="CAP CER 10PF 50V NP0 0603"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C106" library="rc-sysmocom" package="_0603" value="100n">
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics America, Inc"/>
<attribute name="SOURCEPARTNUMBER" value="1276-1005-1-ND"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="LINK" value="http://www.digikey.com/product-detail/en/foo/1276-1005-1-ND"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="MANUFACTURERPARTNUMBER" value="CL10B104KO8NNNC"/>
<attribute name="DESCRIPTION" value="CAP CER 0.1UF 16V 10% X7R 0603"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C111" library="rc-sysmocom" package="_0402" value="33p">
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics America, Inc."/>
<attribute name="SOURCEPARTNUMBER" value="1276-1272-1-ND"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="LINK" value="http://www.digikey.com/product-detail/en/CL05C330JB5NNNC/1276-1272-1-ND/3889358"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="MANUFACTURERPARTNUMBER" value="CL05C330JB5NNNC"/>
<attribute name="DESCRIPTION" value="CAP CER 33PF 50V NP0 0402"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C112" library="rc-sysmocom" package="_0603" value="10p">
<attribute name="MANUFACTURER" value="Kemet"/>
<attribute name="SOURCEPARTNUMBER" value="399-1049-1-ND"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="LINK" value="http://www.digikey.com/product-detail/en/C0603C100J5GACTU/399-1049-1-ND"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="MANUFACTURERPARTNUMBER" value="C0603C100J5GACTU"/>
<attribute name="DESCRIPTION" value="CAP CER 10PF 50V NP0 0603"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C110" library="rc-sysmocom" package="_0603" value="100n">
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics America, Inc"/>
<attribute name="SOURCEPARTNUMBER" value="1276-1005-1-ND"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="LINK" value="http://www.digikey.com/product-detail/en/foo/1276-1005-1-ND"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="MANUFACTURERPARTNUMBER" value="CL10B104KO8NNNC"/>
<attribute name="DESCRIPTION" value="CAP CER 0.1UF 16V 10% X7R 0603"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C105" library="rc-sysmocom" package="1206" value="100u">
<attribute name="MANUFACTURER" value="Murata Electronics North America"/>
<attribute name="SOURCEPARTNUMBER" value="490-7217-1-ND"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="LINK" value="http://www.digikey.com/product-detail/en/murata-electronics-north-america/GRM31CR60J107ME39K/490-7217-1-ND/3991203"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="MANUFACTURERPARTNUMBER" value="GRM31CR60J107ME39K"/>
<attribute name="DESCRIPTION" value="100µF 6.3V Ceramic Capacitor X5R 1206 (3216 Metric) 0.126&quot; L x 0.063&quot; W (3.20mm x 1.60mm)"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C109" library="rc-sysmocom" package="1206" value="100u">
<attribute name="LINK" value="http://www.digikey.com/product-detail/en/murata-electronics-north-america/GRM31CR60J107ME39K/490-7217-1-ND/3991203"/>
<attribute name="DESCRIPTION" value="100µF 6.3V Ceramic Capacitor X5R 1206 (3216 Metric) 0.126&quot; L x 0.063&quot; W (3.20mm x 1.60mm)"/>
<attribute name="MANUFACTURER" value="Murata Electronics North America"/>
<attribute name="MANUFACTURERPARTNUMBER" value="GRM31CR60J107ME39K"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="490-7217-1-ND"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="rc-sysmocom" package="_0402" value="33p">
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics America, Inc."/>
<attribute name="SOURCEPARTNUMBER" value="1276-1272-1-ND"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="LINK" value="http://www.digikey.com/product-detail/en/CL05C330JB5NNNC/1276-1272-1-ND/3889358"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="MANUFACTURERPARTNUMBER" value="CL05C330JB5NNNC"/>
<attribute name="DESCRIPTION" value="CAP CER 33PF 50V NP0 0402"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="rc-sysmocom" package="_0402" value="33p">
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics America, Inc."/>
<attribute name="SOURCEPARTNUMBER" value="1276-1272-1-ND"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="LINK" value="http://www.digikey.com/product-detail/en/CL05C330JB5NNNC/1276-1272-1-ND/3889358"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="MANUFACTURERPARTNUMBER" value="CL05C330JB5NNNC"/>
<attribute name="DESCRIPTION" value="CAP CER 33PF 50V NP0 0402"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="rc-sysmocom" package="_0402" value="33p">
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics America, Inc."/>
<attribute name="SOURCEPARTNUMBER" value="1276-1272-1-ND"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="LINK" value="http://www.digikey.com/product-detail/en/CL05C330JB5NNNC/1276-1272-1-ND/3889358"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="MANUFACTURERPARTNUMBER" value="CL05C330JB5NNNC"/>
<attribute name="DESCRIPTION" value="CAP CER 33PF 50V NP0 0402"/>
<attribute name="SOURCE" value="DIGIKEY"/>
</element>
<element name="JP4" library="pinhead" package="2X12" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="LINK" value="http://www.digikey.com/product-detail/en/961224-6404-AR/3M9463-ND/2071504"/>
<attribute name="DESCRIPTION" value="24 Positions Header, Unshrouded Connector 0.100&quot; (2.54mm) Through Hole Gold"/>
<attribute name="MANUFACTURER" value="3M"/>
<attribute name="MANUFACTURERPARTNUMBER" value="961224-6404-AR"/>
<attribute name="SOURCEPARTNUMBER" value="3M9463-ND"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="CLASS" value="CONNECTOR\JUMPER"/>
</element>
<element name="C8" library="rc-sysmocom" package="_0603" value="100n">
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics America, Inc"/>
<attribute name="SOURCEPARTNUMBER" value="1276-1005-1-ND"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="LINK" value="http://www.digikey.com/product-detail/en/foo/1276-1005-1-ND"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="MANUFACTURERPARTNUMBER" value="CL10B104KO8NNNC"/>
<attribute name="DESCRIPTION" value="CAP CER 0.1UF 16V 10% X7R 0603"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="rc-sysmocom" package="_0603" value="1M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="LINK" value="http://www.digikey.com/product-detail/en/yageo/RC0603JR-071ML/311-1.0MGRCT-ND/729625"/>
<attribute name="DESCRIPTION" value="RES SMD 1M OHM 5% 1/10W 0603"/>
<attribute name="MANUFACTURER" value="Yageo"/>
<attribute name="MANUFACTURERPARTNUMBER" value="RC0603JR-071ML"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="311-1.0MGRCT-ND"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="RESISTOR"/>
</element>
<element name="C9" library="rc-sysmocom" package="_0603" value="100n">
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics America, Inc"/>
<attribute name="SOURCEPARTNUMBER" value="1276-1005-1-ND"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="LINK" value="http://www.digikey.com/product-detail/en/foo/1276-1005-1-ND"/>
<attribute name="ROHSCERTIFICATE" value="Bleifrei / RoHS-konform"/>
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="MANUFACTURERPARTNUMBER" value="CL10B104KO8NNNC"/>
<attribute name="DESCRIPTION" value="CAP CER 0.1UF 16V 10% X7R 0603"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="led" package="CHIP-LED0603" value="GREEN">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="NO DESCRIPTION"/>
<attribute name="MANUFACTURER" value="UNKNOWN MANUFACTURER"/>
<attribute name="MANUFACTURERPARTNUMBER" value="UNKNOWN MANUFACTURER PART NUMBER"/>
<attribute name="SOURCE" value="UNKNOWN SOURCE"/>
<attribute name="SOURCEPARTNUMBER" value="UNKNOWN SOURCE PART NUMBER"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="LED"/>
<attribute name="LINK" value="UNKNOWN LINK"/>
</element>
<element name="R5" library="rc-sysmocom" package="_0603" value="330">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESCRIPTION" value="RES SMD 330 OHM 5% 1/10W 0603"/>
<attribute name="MANUFACTURER" value="Yageo"/>
<attribute name="MANUFACTURERPARTNUMBER" value="RC0603JR-07330RL"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="311-330GRCT-ND"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="RESISTOR"/>
<attribute name="LINK" value="http://www.digikey.com/product-detail/en/yageo/RC0603JR-07330RL/311-330GRCT-ND/729716"/>
</element>
<element name="C10" library="rc-sysmocom" package="1206" value="100u">
<attribute name="LINK" value="http://www.digikey.com/product-detail/en/murata-electronics-north-america/GRM31CR60J107ME39K/490-7217-1-ND/3991203"/>
<attribute name="DESCRIPTION" value="100µF 6.3V Ceramic Capacitor X5R 1206 (3216 Metric) 0.126&quot; L x 0.063&quot; W (3.20mm x 1.60mm)"/>
<attribute name="MANUFACTURER" value="Murata Electronics North America"/>
<attribute name="MANUFACTURERPARTNUMBER" value="GRM31CR60J107ME39K"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="490-7217-1-ND"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="rc-sysmocom" package="1206" value="100u">
<attribute name="LINK" value="http://www.digikey.com/product-detail/en/murata-electronics-north-america/GRM31CR60J107ME39K/490-7217-1-ND/3991203"/>
<attribute name="DESCRIPTION" value="100µF 6.3V Ceramic Capacitor X5R 1206 (3216 Metric) 0.126&quot; L x 0.063&quot; W (3.20mm x 1.60mm)"/>
<attribute name="MANUFACTURER" value="Murata Electronics North America"/>
<attribute name="MANUFACTURERPARTNUMBER" value="GRM31CR60J107ME39K"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="490-7217-1-ND"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="CAPACITOR"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="rc-sysmocom" package="_0603" value="330">
<attribute name="LINK" value="http://www.digikey.com/product-detail/en/yageo/RC0603JR-07330RL/311-330GRCT-ND/729716"/>
<attribute name="MANUFACTURERPARTNUMBER" value="RC0603JR-07330RL"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="CLASS" value="RESISTOR"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="MANUFACTURER" value="Yageo"/>
<attribute name="SOURCEPARTNUMBER" value="311-330GRCT-ND"/>
<attribute name="DESCRIPTION" value="RES SMD 330 OHM 5% 1/10W 0603"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X3" library="laforge" package="SMA-F-S-TH" value="">
<attribute name="DESCRIPTION" value="CONN SMA JACK STR 50 OHM PCB"/>
<attribute name="MANUFACTURER" value="TE Connectivity AMP Connectors"/>
<attribute name="MANUFACTURERPARTNUMBER" value="5-1814832-1"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="A97594-ND"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="CONNECTOR"/>
<attribute name="LINK" value="http://www.digikey.com/product-detail/en/te-connectivity-amp-connectors/5-1814832-1/A97594-ND/1755982"/>
</element>
<element name="X4" library="laforge" package="SMA-F-S-TH" value="">
<attribute name="DESCRIPTION" value="CONN SMA JACK STR 50 OHM PCB"/>
<attribute name="MANUFACTURER" value="TE Connectivity AMP Connectors"/>
<attribute name="MANUFACTURERPARTNUMBER" value="5-1814832-1"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="A97594-ND"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="CONNECTOR"/>
<attribute name="LINK" value="http://www.digikey.com/product-detail/en/te-connectivity-amp-connectors/5-1814832-1/A97594-ND/1755982"/>
</element>
<element name="Y3" library="laforge" package="HRS_UFL" value="">
<attribute name="OC_DIGIKEY" value="H9161CT-ND"/>
<attribute name="DESCRIPTION" value="CONN UMC RCPT STR 50 OHM SMD"/>
<attribute name="MANUFACTURER" value="Hirose Electric Co Ltd"/>
<attribute name="MANUFACTURERPARTNUMBER" value="U.FL-R-SMT(01)"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="H9161-ND"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="UNKNOWN CLASS"/>
<attribute name="LINK" value="http://www.digikey.com/product-detail/en/hirose-electric-co-ltd/U.FL-R-SMT(01)/H9161-ND/513010"/>
</element>
<element name="Y4" library="laforge" package="HRS_UFL" value="">
<attribute name="OC_DIGIKEY" value="H9161CT-ND"/>
<attribute name="DESCRIPTION" value="CONN UMC RCPT STR 50 OHM SMD"/>
<attribute name="MANUFACTURER" value="Hirose Electric Co Ltd"/>
<attribute name="MANUFACTURERPARTNUMBER" value="U.FL-R-SMT(01)"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="H9161-ND"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="UNKNOWN CLASS"/>
<attribute name="LINK" value="http://www.digikey.com/product-detail/en/hirose-electric-co-ltd/U.FL-R-SMT(01)/H9161-ND/513010"/>
</element>
<element name="X5" library="laforge" package="SMA-F-S-TH" value="">
<attribute name="DESCRIPTION" value="CONN SMA JACK STR 50 OHM PCB"/>
<attribute name="MANUFACTURER" value="TE Connectivity AMP Connectors"/>
<attribute name="MANUFACTURERPARTNUMBER" value="5-1814832-1"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="A97594-ND"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="CONNECTOR"/>
<attribute name="LINK" value="http://www.digikey.com/product-detail/en/te-connectivity-amp-connectors/5-1814832-1/A97594-ND/1755982"/>
</element>
<element name="Y5" library="laforge" package="HRS_UFL" value="">
<attribute name="OC_DIGIKEY" value="H9161CT-ND"/>
<attribute name="DESCRIPTION" value="CONN UMC RCPT STR 50 OHM SMD"/>
<attribute name="MANUFACTURER" value="Hirose Electric Co Ltd"/>
<attribute name="MANUFACTURERPARTNUMBER" value="U.FL-R-SMT(01)"/>
<attribute name="SOURCE" value="DIGIKEY"/>
<attribute name="SOURCEPARTNUMBER" value="H9161-ND"/>
<attribute name="ROHSCERTIFICATE" value="UNKNOWN ROHS CERTIFICATE"/>
<attribute name="POPULATED" value="TRUE"/>
<attribute name="CLASS" value="UNKNOWN CLASS"/>
<attribute name="LINK" value="http://www.digikey.com/product-detail/en/hirose-electric-co-ltd/U.FL-R-SMT(01)/H9161-ND/513010"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="X1" pad="9"/>
<contactref element="X1" pad="43"/>
<contactref element="X1" pad="37"/>
<contactref element="X1" pad="35"/>
<contactref element="X1" pad="29"/>
<contactref element="X1" pad="27"/>
<contactref element="X1" pad="21"/>
<contactref element="X1" pad="15"/>
<contactref element="X1" pad="18"/>
<contactref element="X1" pad="4"/>
<contactref element="X1" pad="26"/>
<contactref element="X1" pad="34"/>
<contactref element="X1" pad="40"/>
<contactref element="X1" pad="50"/>
<contactref element="SIM1" pad="5"/>
<contactref element="JP1" pad="2"/>
<contactref element="U2" pad="LEFT"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="K1" pad="3"/>
<contactref element="K1" pad="2"/>
<contactref element="U1" pad="2"/>
<contactref element="X2" pad="5"/>
<contactref element="C3" pad="-"/>
<contactref element="C4" pad="-"/>
<contactref element="C107" pad="2"/>
<contactref element="C106" pad="1"/>
<contactref element="C108" pad="2"/>
<contactref element="C105" pad="1"/>
<contactref element="C111" pad="2"/>
<contactref element="C110" pad="1"/>
<contactref element="C112" pad="2"/>
<contactref element="C109" pad="1"/>
<contactref element="C6" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="JP2" pad="1"/>
<contactref element="JP4" pad="1"/>
<contactref element="JP4" pad="13"/>
<contactref element="C8" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="X3" pad="G1"/>
<contactref element="Y3" pad="GND@1"/>
<contactref element="X3" pad="G2"/>
<contactref element="X3" pad="G3"/>
<contactref element="X3" pad="G4"/>
<contactref element="Y3" pad="GND@2"/>
<contactref element="X4" pad="G1"/>
<contactref element="Y4" pad="GND@1"/>
<contactref element="X4" pad="G2"/>
<contactref element="X4" pad="G3"/>
<contactref element="X4" pad="G4"/>
<contactref element="Y4" pad="GND@2"/>
<contactref element="X5" pad="G1"/>
<contactref element="Y5" pad="GND@1"/>
<contactref element="X5" pad="G2"/>
<contactref element="X5" pad="G3"/>
<contactref element="X5" pad="G4"/>
<contactref element="Y5" pad="GND@2"/>
</signal>
<signal name="USIM_POWER">
<contactref element="X1" pad="8"/>
<contactref element="SIM1" pad="1"/>
<contactref element="C8" pad="2"/>
</signal>
<signal name="USIM_DATA">
<contactref element="SIM1" pad="7"/>
<contactref element="R1" pad="2"/>
<contactref element="C7" pad="1"/>
</signal>
<signal name="USIM_CLK">
<contactref element="SIM1" pad="3"/>
<contactref element="R2" pad="2"/>
<contactref element="C5" pad="1"/>
</signal>
<signal name="USIM_RESET">
<contactref element="SIM1" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="C6" pad="1"/>
</signal>
<signal name="USIM_VPP">
<contactref element="X1" pad="16"/>
<contactref element="SIM1" pad="6"/>
</signal>
<signal name="VDD_1V5">
<contactref element="X1" pad="48"/>
<contactref element="X1" pad="28"/>
<contactref element="X1" pad="6"/>
</signal>
<signal name="VCC_3V3">
<contactref element="X1" pad="39"/>
<contactref element="X1" pad="41"/>
<contactref element="X1" pad="52"/>
<contactref element="X1" pad="24"/>
<contactref element="X1" pad="2"/>
<contactref element="LED1" pad="A"/>
<contactref element="U2" pad="PAD"/>
<contactref element="C2" pad="2"/>
<contactref element="C4" pad="+"/>
<contactref element="C111" pad="1"/>
<contactref element="C110" pad="2"/>
<contactref element="C112" pad="1"/>
<contactref element="C107" pad="1"/>
<contactref element="C106" pad="2"/>
<contactref element="C108" pad="1"/>
<contactref element="C105" pad="2"/>
<contactref element="C109" pad="2"/>
<contactref element="JP4" pad="14"/>
<contactref element="LED2" pad="A"/>
<contactref element="C10" pad="2"/>
<contactref element="C11" pad="2"/>
</signal>
<signal name="USB_D_N">
<contactref element="X1" pad="36"/>
<contactref element="U1" pad="4"/>
</signal>
<signal name="USB_D_P">
<contactref element="X1" pad="38"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="UIM_C8">
<contactref element="X1" pad="17"/>
<contactref element="JP4" pad="7"/>
</signal>
<signal name="UIM_C4">
<contactref element="X1" pad="19"/>
<contactref element="JP4" pad="10"/>
</signal>
<signal name="N$3">
<contactref element="X1" pad="42"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="PERST">
<contactref element="X1" pad="22"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="W_DISABLE">
<contactref element="X1" pad="20"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="X1" pad="10"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="X1" pad="12"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="X1" pad="14"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="X2" pad="M1"/>
<contactref element="X2" pad="M4"/>
<contactref element="X2" pad="M3"/>
<contactref element="X2" pad="M2"/>
<contactref element="C9" pad="2"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="LDO_IN">
<contactref element="U2" pad="RIGHT"/>
<contactref element="C1" pad="2"/>
<contactref element="JP3" pad="2"/>
<contactref element="C3" pad="+"/>
</signal>
<signal name="N$12">
<contactref element="K1" pad="1-1"/>
<contactref element="K1" pad="1"/>
<contactref element="JP3" pad="3"/>
</signal>
<signal name="USB_VBUS">
<contactref element="JP3" pad="1"/>
<contactref element="U1" pad="5"/>
<contactref element="X2" pad="1"/>
</signal>
<signal name="WAKE">
<contactref element="X1" pad="1"/>
<contactref element="JP4" pad="2"/>
</signal>
<signal name="COEX1">
<contactref element="X1" pad="3"/>
<contactref element="JP4" pad="4"/>
</signal>
<signal name="COEX2">
<contactref element="X1" pad="5"/>
<contactref element="JP4" pad="3"/>
</signal>
<signal name="!CLKREQ">
<contactref element="X1" pad="7"/>
<contactref element="JP4" pad="6"/>
</signal>
<signal name="REFCLK-">
<contactref element="X1" pad="11"/>
<contactref element="JP4" pad="5"/>
</signal>
<signal name="REFCLK+">
<contactref element="X1" pad="13"/>
<contactref element="JP4" pad="8"/>
</signal>
<signal name="PERN0">
<contactref element="X1" pad="23"/>
<contactref element="JP4" pad="9"/>
</signal>
<signal name="PERP0">
<contactref element="X1" pad="25"/>
<contactref element="JP4" pad="12"/>
</signal>
<signal name="PETN0">
<contactref element="X1" pad="31"/>
<contactref element="JP4" pad="16"/>
</signal>
<signal name="PETP0">
<contactref element="X1" pad="33"/>
<contactref element="JP4" pad="15"/>
</signal>
<signal name="RSVRD45">
<contactref element="X1" pad="45"/>
<contactref element="JP4" pad="18"/>
</signal>
<signal name="RSVRD47">
<contactref element="X1" pad="47"/>
<contactref element="JP4" pad="17"/>
</signal>
<signal name="RSVRD49">
<contactref element="X1" pad="49"/>
<contactref element="JP4" pad="20"/>
</signal>
<signal name="RSVRD51">
<contactref element="X1" pad="51"/>
<contactref element="JP4" pad="19"/>
</signal>
<signal name="LED_WPAN">
<contactref element="X1" pad="46"/>
<contactref element="JP4" pad="23"/>
</signal>
<signal name="LED_WLAN">
<contactref element="X1" pad="44"/>
<contactref element="JP4" pad="24"/>
</signal>
<signal name="SMB_DATA">
<contactref element="X1" pad="32"/>
<contactref element="JP4" pad="22"/>
</signal>
<signal name="SMB_CLK">
<contactref element="X1" pad="30"/>
<contactref element="JP4" pad="21"/>
</signal>
<signal name="N$16">
<contactref element="JP4" pad="11"/>
</signal>
<signal name="_USB_D_N">
<contactref element="X2" pad="2"/>
<contactref element="U1" pad="6"/>
</signal>
<signal name="_USB_D_P">
<contactref element="X2" pad="3"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="LED2" pad="C"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="LED1" pad="C"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="X3" pad="C"/>
<contactref element="Y3" pad="SIG"/>
</signal>
<signal name="N$14">
<contactref element="X4" pad="C"/>
<contactref element="Y4" pad="SIG"/>
</signal>
<signal name="N$7">
<contactref element="X5" pad="C"/>
<contactref element="Y5" pad="SIG"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
