<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<library>
<packages>
<package name="R-PDSO-G14">
<description>TI TSSOP14 package</description>
</package>
<package name="SOIC14">
<description>SOIC-14</description>
</package>
</packages>
<symbols>
<symbol name="SN65LVDS1">
<description>Differential Line Driver and Receiver w/ individual EN pin</description>
<pin name="D" direction="in"/>
<pin name="Y" direction="out"/>
<pin name="Z" direction="out"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="DE" direction="in"/>
<pin name="R" direction="out"/>
<pin name="RE" direction="in"/>
</symbol>
<symbol name="2PWR2GND">
<description>2PWR2GND</description>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="SN65LVDS180" prefix="IC">
<description>High-Speed Differential Line Drivers and Receivers</description>
<gates>
<gate name="-XCVR" symbol="SN65LVDS1"/>
<gate name="-PWR" symbol="2PWR2GND"/>
</gates>
<devices>
<device name="D" package="SOIC14">
<connects>
<connect gate="-PWR" pin="GND@1" pad="6"/>
<connect gate="-PWR" pin="GND@2" pad="7"/>
<connect gate="-PWR" pin="VCC@1" pad="13"/>
<connect gate="-PWR" pin="VCC@2" pad="14"/>
<connect gate="-XCVR" pin="A" pad="12"/>
<connect gate="-XCVR" pin="B" pad="11"/>
<connect gate="-XCVR" pin="D" pad="5"/>
<connect gate="-XCVR" pin="DE" pad="4"/>
<connect gate="-XCVR" pin="R" pad="2"/>
<connect gate="-XCVR" pin="RE" pad="3"/>
<connect gate="-XCVR" pin="Y" pad="9"/>
<connect gate="-XCVR" pin="Z" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PW" package="R-PDSO-G14">
<connects>
<connect gate="-PWR" pin="GND@1" pad="6"/>
<connect gate="-PWR" pin="GND@2" pad="7"/>
<connect gate="-PWR" pin="VCC@1" pad="13"/>
<connect gate="-PWR" pin="VCC@2" pad="14"/>
<connect gate="-XCVR" pin="A" pad="12"/>
<connect gate="-XCVR" pin="B" pad="11"/>
<connect gate="-XCVR" pin="D" pad="5"/>
<connect gate="-XCVR" pin="DE" pad="4"/>
<connect gate="-XCVR" pin="R" pad="2"/>
<connect gate="-XCVR" pin="RE" pad="3"/>
<connect gate="-XCVR" pin="Y" pad="9"/>
<connect gate="-XCVR" pin="Z" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
