<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<library>
<description>
</description>
<packages>
<package name="SOT23-5">
<description>SOT23-5</description>
</package>
<package name="SO08N">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt; SOIC 150 mil</description>
</package>
</packages>
<symbols>
<symbol name="SN65LVDT2">
<description>Single LVDS Receiver</description>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="R" direction="out"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="SN65LVDT2" prefix="IC">
<description>Single LVDS Receiver</description>
<gates>
<gate name="A" symbol="SN65LVDT2"/>
</gates>
<devices>
<device name="D" package="SO08N">
<connects>
<connect gate="A" pin="A" pad="2"/>
<connect gate="A" pin="B" pad="1"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="R" pad="7"/>
<connect gate="A" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DBV" package="SOT23-5">
<connects>
<connect gate="A" pin="A" pad="3"/>
<connect gate="A" pin="B" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="R" pad="5"/>
<connect gate="A" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
